<?xml version="1.0" encoding="utf-8" standalone="no"?>
<device schemaVersion="1.1"
xmlns:xs="http://www.w3.org/2001/XMLSchema-instance"
xs:noNamespaceSchemaLocation="CMSIS-SVD_Schema_1_1.xsd">
  <name>STM32L0x3</name>
  <version>1.0</version>
  <description>STM32L0x3</description>
  <!--Bus Interface Properties-->
  <!--Cortex-M3 is byte addressable-->
  <addressUnitBits>8</addressUnitBits>
  <!--the maximum data bit width accessible within a single transfer-->
  <width>32</width>
  <!--Register Default Properties-->
  <size>0x20</size>
  <resetValue>0x0</resetValue>
  <resetMask>0xFFFFFFFF</resetMask>
  <peripherals>
    <peripheral>
      <name>AES</name>
      <description>Advanced encryption standard hardware
      accelerator</description>
      <groupName>AES</groupName>
      <baseAddress>0x40026000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>AES_RNG_LPUART1</name>
        <description>AES global interrupt RNG global interrupt and
        LPUART1 global interrupt through</description>
        <value>29</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DMAOUTEN</name>
              <description>Enable DMA management of data output
              phase</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAINEN</name>
              <description>Enable DMA management of data input
              phase</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupt enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CCFIE</name>
              <description>CCF flag interrupt enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRC</name>
              <description>Error clear</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CCFC</name>
              <description>Computation Complete Flag
              Clear</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHMOD</name>
              <description>AES chaining mode</description>
              <bitOffset>5</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE</name>
              <description>AES operating mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DATATYPE</name>
              <description>Data type selection (for data in and
              data out to/from the cryptographic
              block)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>AES enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>WRERR</name>
              <description>Write error flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RDERR</name>
              <description>Read error flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CCF</name>
              <description>Computation complete flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DINR</name>
          <displayName>DINR</displayName>
          <description>data input register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_DINR</name>
              <description>Data Input Register.</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DOUTR</name>
          <displayName>DOUTR</displayName>
          <description>data output register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_DOUTR</name>
              <description>Data output register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>KEYR0</name>
          <displayName>KEYR0</displayName>
          <description>key register 0</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_KEYR0</name>
              <description>Data Output Register (LSB key
              [31:0])</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>KEYR1</name>
          <displayName>KEYR1</displayName>
          <description>key register 1</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_KEYR1</name>
              <description>AES key register (key
              [63:32])</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>KEYR2</name>
          <displayName>KEYR2</displayName>
          <description>key register 2</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_KEYR2</name>
              <description>AES key register (key
              [95:64])</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>KEYR3</name>
          <displayName>KEYR3</displayName>
          <description>key register 3</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_KEYR3</name>
              <description>AES key register (MSB key
              [127:96])</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IVR0</name>
          <displayName>IVR0</displayName>
          <description>initialization vector register
          0</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_IVR0</name>
              <description>initialization vector register (LSB IVR
              [31:0])</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IVR1</name>
          <displayName>IVR1</displayName>
          <description>initialization vector register
          1</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_IVR1</name>
              <description>Initialization Vector Register (IVR
              [63:32])</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IVR2</name>
          <displayName>IVR2</displayName>
          <description>initialization vector register
          2</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_IVR2</name>
              <description>Initialization Vector Register (IVR
              [95:64])</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IVR3</name>
          <displayName>IVR3</displayName>
          <description>initialization vector register
          3</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AES_IVR3</name>
              <description>Initialization Vector Register (MSB IVR
              [127:96])</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>DAC</name>
      <description>Digital-to-analog converter</description>
      <groupName>DAC</groupName>
      <baseAddress>0x40007400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DMAUDRIE1</name>
              <description>DAC channel1 DMA Underrun Interrupt
              enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAEN1</name>
              <description>DAC channel1 DMA enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MAMP1</name>
              <description>DAC channel1 mask/amplitude
              selector</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>WAVE1</name>
              <description>DAC channel1 noise/triangle wave
              generation enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TSEL1</name>
              <description>DAC channel1 trigger
              selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TEN1</name>
              <description>DAC channel1 trigger
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BOFF1</name>
              <description>DAC channel1 output buffer
              disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN1</name>
              <description>DAC channel1 enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SWTRIGR</name>
          <displayName>SWTRIGR</displayName>
          <description>software trigger register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SWTRIG1</name>
              <description>DAC channel1 software
              trigger</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12R1</name>
          <displayName>DHR12R1</displayName>
          <description>channel1 12-bit right-aligned data holding
          register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 12-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12L1</name>
          <displayName>DHR12L1</displayName>
          <description>channel1 12-bit left-aligned data holding
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 12-bit left-aligned
              data</description>
              <bitOffset>4</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR8R1</name>
          <displayName>DHR8R1</displayName>
          <description>channel1 8-bit right-aligned data holding
          register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 8-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DOR1</name>
          <displayName>DOR1</displayName>
          <description>channel1 data output register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DOR</name>
              <description>DAC channel1 data output</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DMAUDR1</name>
              <description>DAC channel1 DMA underrun
              flag</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12R2</name>
          <displayName>DHR12R2</displayName>
          <description>channel2 12-bit right-aligned data holding
          register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 12-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12L2</name>
          <displayName>DHR12L2</displayName>
          <description>channel2 12-bit left-aligned data holding
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 12-bit left-aligned
              data</description>
              <bitOffset>4</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR8R2</name>
          <displayName>DHR8R2</displayName>
          <description>channel2 8-bit right-aligned data holding
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 8-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12RD</name>
          <displayName>DHR12RD</displayName>
          <description>Dual DAC 12-bit right-aligned data holding
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 12-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 12-bit right-aligned
              data</description>
              <bitOffset>16</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12LD</name>
          <displayName>DHR12LD</displayName>
          <description>Dual DAC 12-bit left-aligned data holding
          register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 12-bit left-aligned
              data</description>
              <bitOffset>4</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 12-bit left-aligned
              data</description>
              <bitOffset>20</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR8RD</name>
          <displayName>DHR8RD</displayName>
          <description>Dual DAC 8-bit right-aligned data holding
          register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 8-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 8-bit right-aligned
              data</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DOR2</name>
          <displayName>DOR2</displayName>
          <description>channel2 data output register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DOR</name>
              <description>DAC channel2 data output</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>DMA1</name>
      <description>Direct memory access controller</description>
      <groupName>DMA</groupName>
      <baseAddress>0x40020000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>DMA1_Channel1</name>
        <description>DMA1 Channel1 global interrupt</description>
        <value>9</value>
      </interrupt>
      <interrupt>
        <name>DMA1_Channel2_3</name>
        <description>DMA1 Channel2 and 3 interrupts</description>
        <value>10</value>
      </interrupt>
      <interrupt>
        <name>DMA1_Channel4_7</name>
        <description>DMA1 Channel4 to 7 interrupts</description>
        <value>11</value>
      </interrupt>
      <registers>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>interrupt status register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TEIF7</name>
              <description>Channel x transfer error flag (x = 1
              ..7)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF7</name>
              <description>Channel x half transfer flag (x = 1
              ..7)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF7</name>
              <description>Channel x transfer complete flag (x = 1
              ..7)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GIF7</name>
              <description>Channel x global interrupt flag (x = 1
              ..7)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF6</name>
              <description>Channel x transfer error flag (x = 1
              ..7)</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF6</name>
              <description>Channel x half transfer flag (x = 1
              ..7)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF6</name>
              <description>Channel x transfer complete flag (x = 1
              ..7)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GIF6</name>
              <description>Channel x global interrupt flag (x = 1
              ..7)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF5</name>
              <description>Channel x transfer error flag (x = 1
              ..7)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF5</name>
              <description>Channel x half transfer flag (x = 1
              ..7)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF5</name>
              <description>Channel x transfer complete flag (x = 1
              ..7)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GIF5</name>
              <description>Channel x global interrupt flag (x = 1
              ..7)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF4</name>
              <description>Channel x transfer error flag (x = 1
              ..7)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF4</name>
              <description>Channel x half transfer flag (x = 1
              ..7)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF4</name>
              <description>Channel x transfer complete flag (x = 1
              ..7)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GIF4</name>
              <description>Channel x global interrupt flag (x = 1
              ..7)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF3</name>
              <description>Channel x transfer error flag (x = 1
              ..7)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF3</name>
              <description>Channel x half transfer flag (x = 1
              ..7)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF3</name>
              <description>Channel x transfer complete flag (x = 1
              ..7)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GIF3</name>
              <description>Channel x global interrupt flag (x = 1
              ..7)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF2</name>
              <description>Channel x transfer error flag (x = 1
              ..7)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF2</name>
              <description>Channel x half transfer flag (x = 1
              ..7)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF2</name>
              <description>Channel x transfer complete flag (x = 1
              ..7)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GIF2</name>
              <description>Channel x global interrupt flag (x = 1
              ..7)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF1</name>
              <description>Channel x transfer error flag (x = 1
              ..7)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF1</name>
              <description>Channel x half transfer flag (x = 1
              ..7)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF1</name>
              <description>Channel x transfer complete flag (x = 1
              ..7)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GIF1</name>
              <description>Channel x global interrupt flag (x = 1
              ..7)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IFCR</name>
          <displayName>IFCR</displayName>
          <description>interrupt flag clear register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CTEIF7</name>
              <description>Channel x transfer error clear (x = 1
              ..7)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF7</name>
              <description>Channel x half transfer clear (x = 1
              ..7)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF7</name>
              <description>Channel x transfer complete clear (x = 1
              ..7)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CGIF7</name>
              <description>Channel x global interrupt clear (x = 1
              ..7)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF6</name>
              <description>Channel x transfer error clear (x = 1
              ..7)</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF6</name>
              <description>Channel x half transfer clear (x = 1
              ..7)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF6</name>
              <description>Channel x transfer complete clear (x = 1
              ..7)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CGIF6</name>
              <description>Channel x global interrupt clear (x = 1
              ..7)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF5</name>
              <description>Channel x transfer error clear (x = 1
              ..7)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF5</name>
              <description>Channel x half transfer clear (x = 1
              ..7)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF5</name>
              <description>Channel x transfer complete clear (x = 1
              ..7)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CGIF5</name>
              <description>Channel x global interrupt clear (x = 1
              ..7)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF4</name>
              <description>Channel x transfer error clear (x = 1
              ..7)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF4</name>
              <description>Channel x half transfer clear (x = 1
              ..7)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF4</name>
              <description>Channel x transfer complete clear (x = 1
              ..7)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CGIF4</name>
              <description>Channel x global interrupt clear (x = 1
              ..7)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF3</name>
              <description>Channel x transfer error clear (x = 1
              ..7)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF3</name>
              <description>Channel x half transfer clear (x = 1
              ..7)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF3</name>
              <description>Channel x transfer complete clear (x = 1
              ..7)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CGIF3</name>
              <description>Channel x global interrupt clear (x = 1
              ..7)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF2</name>
              <description>Channel x transfer error clear (x = 1
              ..7)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF2</name>
              <description>Channel x half transfer clear (x = 1
              ..7)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF2</name>
              <description>Channel x transfer complete clear (x = 1
              ..7)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CGIF2</name>
              <description>Channel x global interrupt clear (x = 1
              ..7)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF1</name>
              <description>Channel x transfer error clear (x = 1
              ..7)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF1</name>
              <description>Channel x half transfer clear (x = 1
              ..7)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF1</name>
              <description>Channel x transfer complete clear (x = 1
              ..7)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CGIF1</name>
              <description>Channel x global interrupt clear (x = 1
              ..7)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <displayName>CCR1</displayName>
          <description>channel x configuration
          register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MEM2MEM</name>
              <description>Memory to memory mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Channel priority level</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory size</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral size</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Channel enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNDTR1</name>
          <displayName>CNDTR1</displayName>
          <description>channel x number of data
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data to transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CPAR1</name>
          <displayName>CPAR1</displayName>
          <description>channel x peripheral address
          register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMAR1</name>
          <displayName>CMAR1</displayName>
          <description>channel x memory address
          register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MA</name>
              <description>Memory address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR2</name>
          <displayName>CCR2</displayName>
          <description>channel x configuration
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MEM2MEM</name>
              <description>Memory to memory mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Channel priority level</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory size</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral size</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Channel enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNDTR2</name>
          <displayName>CNDTR2</displayName>
          <description>channel x number of data
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data to transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CPAR2</name>
          <displayName>CPAR2</displayName>
          <description>channel x peripheral address
          register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMAR2</name>
          <displayName>CMAR2</displayName>
          <description>channel x memory address
          register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MA</name>
              <description>Memory address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR3</name>
          <displayName>CCR3</displayName>
          <description>channel x configuration
          register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MEM2MEM</name>
              <description>Memory to memory mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Channel priority level</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory size</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral size</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Channel enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNDTR3</name>
          <displayName>CNDTR3</displayName>
          <description>channel x number of data
          register</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data to transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CPAR3</name>
          <displayName>CPAR3</displayName>
          <description>channel x peripheral address
          register</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMAR3</name>
          <displayName>CMAR3</displayName>
          <description>channel x memory address
          register</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MA</name>
              <description>Memory address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR4</name>
          <displayName>CCR4</displayName>
          <description>channel x configuration
          register</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MEM2MEM</name>
              <description>Memory to memory mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Channel priority level</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory size</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral size</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Channel enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNDTR4</name>
          <displayName>CNDTR4</displayName>
          <description>channel x number of data
          register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data to transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CPAR4</name>
          <displayName>CPAR4</displayName>
          <description>channel x peripheral address
          register</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMAR4</name>
          <displayName>CMAR4</displayName>
          <description>channel x memory address
          register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MA</name>
              <description>Memory address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR5</name>
          <displayName>CCR5</displayName>
          <description>channel x configuration
          register</description>
          <addressOffset>0x58</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MEM2MEM</name>
              <description>Memory to memory mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Channel priority level</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory size</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral size</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Channel enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNDTR5</name>
          <displayName>CNDTR5</displayName>
          <description>channel x number of data
          register</description>
          <addressOffset>0x5C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data to transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CPAR5</name>
          <displayName>CPAR5</displayName>
          <description>channel x peripheral address
          register</description>
          <addressOffset>0x60</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMAR5</name>
          <displayName>CMAR5</displayName>
          <description>channel x memory address
          register</description>
          <addressOffset>0x64</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MA</name>
              <description>Memory address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR6</name>
          <displayName>CCR6</displayName>
          <description>channel x configuration
          register</description>
          <addressOffset>0x6C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MEM2MEM</name>
              <description>Memory to memory mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Channel priority level</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory size</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral size</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Channel enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNDTR6</name>
          <displayName>CNDTR6</displayName>
          <description>channel x number of data
          register</description>
          <addressOffset>0x70</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data to transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CPAR6</name>
          <displayName>CPAR6</displayName>
          <description>channel x peripheral address
          register</description>
          <addressOffset>0x74</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMAR6</name>
          <displayName>CMAR6</displayName>
          <description>channel x memory address
          register</description>
          <addressOffset>0x78</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MA</name>
              <description>Memory address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR7</name>
          <displayName>CCR7</displayName>
          <description>channel x configuration
          register</description>
          <addressOffset>0x80</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MEM2MEM</name>
              <description>Memory to memory mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Channel priority level</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory size</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral size</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Channel enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNDTR7</name>
          <displayName>CNDTR7</displayName>
          <description>channel x number of data
          register</description>
          <addressOffset>0x84</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data to transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CPAR7</name>
          <displayName>CPAR7</displayName>
          <description>channel x peripheral address
          register</description>
          <addressOffset>0x88</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMAR7</name>
          <displayName>CMAR7</displayName>
          <description>channel x memory address
          register</description>
          <addressOffset>0x8C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MA</name>
              <description>Memory address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CSELR</name>
          <displayName>CSELR</displayName>
          <description>channel selection register</description>
          <addressOffset>0xA8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>C7S</name>
              <description>DMA channel 7 selection</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>C6S</name>
              <description>DMA channel 6 selection</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>C5S</name>
              <description>DMA channel 5 selection</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>C4S</name>
              <description>DMA channel 4 selection</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>C3S</name>
              <description>DMA channel 3 selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>C2S</name>
              <description>DMA channel 2 selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>C1S</name>
              <description>DMA channel 1 selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>CRC</name>
      <description>Cyclic redundancy check calculation
      unit</description>
      <groupName>CRC</groupName>
      <baseAddress>0x40023000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0xFFFFFFFF</resetValue>
          <fields>
            <field>
              <name>DR</name>
              <description>Data register bits</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>Independent data register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IDR</name>
              <description>General-purpose 8-bit data register
              bits</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>REV_OUT</name>
              <description>Reverse output data</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>REV_IN</name>
              <description>Reverse input data</description>
              <bitOffset>5</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>POLYSIZE</name>
              <description>Polynomial size</description>
              <bitOffset>3</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RESET</name>
              <description>RESET bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>INIT</name>
          <displayName>INIT</displayName>
          <description>Initial CRC value</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0xFFFFFFFF</resetValue>
          <fields>
            <field>
              <name>CRC_INIT</name>
              <description>Programmable initial CRC
              value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>POL</name>
          <displayName>POL</displayName>
          <description>polynomial</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x04C11DB7</resetValue>
          <fields>
            <field>
              <name>Polynomialcoefficients</name>
              <description>Programmable polynomial</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>GPIOA</name>
      <description>General-purpose I/Os</description>
      <groupName>GPIO</groupName>
      <baseAddress>0x50000000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MODER</name>
          <displayName>MODER</displayName>
          <description>GPIO port mode register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0xEBFFFCFF</resetValue>
          <fields>
            <field>
              <name>MODE0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OTYPER</name>
          <displayName>OTYPER</displayName>
          <description>GPIO port output type register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OT15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OSPEEDR</name>
          <displayName>OSPEEDR</displayName>
          <description>GPIO port output speed
          register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OSPEED15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PUPDR</name>
          <displayName>PUPDR</displayName>
          <description>GPIO port pull-up/pull-down
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x24000000</resetValue>
          <fields>
            <field>
              <name>PUPD15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>GPIO port input data register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ID15</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID14</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID13</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID12</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID11</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID10</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID9</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID8</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID7</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID6</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID5</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID4</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID3</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID2</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID1</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID0</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ODR</name>
          <displayName>ODR</displayName>
          <description>GPIO port output data register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OD15</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD14</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD13</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD12</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD11</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD10</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD9</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD8</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD7</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD6</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD5</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD4</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD3</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD2</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD1</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD0</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BSRR</name>
          <displayName>BSRR</displayName>
          <description>GPIO port bit set/reset
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BR15</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR14</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR13</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR12</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR11</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR10</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR9</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR8</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS15</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS14</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS13</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS12</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS11</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS10</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS9</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS8</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS7</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS6</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS5</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS4</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS3</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS2</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS1</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS0</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>LCKR</name>
          <displayName>LCKR</displayName>
          <description>GPIO port configuration lock
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LCKK</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK15</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK14</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK13</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK12</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK11</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK10</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK9</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK8</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK7</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK6</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK5</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK4</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK3</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK2</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK1</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK0</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRL</name>
          <displayName>AFRL</displayName>
          <description>GPIO alternate function low
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFSEL7</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL6</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL5</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL4</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL3</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL2</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL1</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL0</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRH</name>
          <displayName>AFRH</displayName>
          <description>GPIO alternate function high
          register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFSEL15</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL14</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL13</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL12</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL11</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL10</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL9</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL8</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>GPIO port bit reset register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BR15</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR14</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR13</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR12</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR11</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR10</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR9</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR8</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>GPIOB</name>
      <description>General-purpose I/Os</description>
      <groupName>GPIO</groupName>
      <baseAddress>0x50000400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MODER</name>
          <displayName>MODER</displayName>
          <description>GPIO port mode register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0xFFFFFFFF</resetValue>
          <fields>
            <field>
              <name>MODE15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODE0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OTYPER</name>
          <displayName>OTYPER</displayName>
          <description>GPIO port output type register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OT15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OSPEEDR</name>
          <displayName>OSPEEDR</displayName>
          <description>GPIO port output speed
          register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OSPEED15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEED0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PUPDR</name>
          <displayName>PUPDR</displayName>
          <description>GPIO port pull-up/pull-down
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PUPD15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPD0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>GPIO port input data register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ID15</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID14</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID13</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID12</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID11</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID10</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID9</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID8</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID7</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID6</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID5</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID4</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID3</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID2</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID1</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ID0</name>
              <description>Port input data bit (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ODR</name>
          <displayName>ODR</displayName>
          <description>GPIO port output data register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OD15</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD14</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD13</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD12</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD11</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD10</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD9</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD8</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD7</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD6</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD5</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD4</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD3</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD2</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD1</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OD0</name>
              <description>Port output data bit (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BSRR</name>
          <displayName>BSRR</displayName>
          <description>GPIO port bit set/reset
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BR15</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR14</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR13</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR12</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR11</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR10</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR9</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR8</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS15</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS14</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS13</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS12</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS11</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS10</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS9</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS8</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS7</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS6</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS5</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS4</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS3</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS2</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS1</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS0</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>LCKR</name>
          <displayName>LCKR</displayName>
          <description>GPIO port configuration lock
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LCKK</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK15</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK14</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK13</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK12</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK11</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK10</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK9</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK8</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK7</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK6</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK5</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK4</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK3</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK2</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK1</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK0</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRL</name>
          <displayName>AFRL</displayName>
          <description>GPIO alternate function low
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFSEL7</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL6</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL5</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL4</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL3</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL2</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL1</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL0</name>
              <description>Alternate function selection for port x
              pin y (y = 0..7)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRH</name>
          <displayName>AFRH</displayName>
          <description>GPIO alternate function high
          register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFSEL15</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL14</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL13</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL12</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL11</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL10</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL9</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFSEL8</name>
              <description>Alternate function selection for port x
              pin y (y = 8..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>GPIO port bit reset register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BR15</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR14</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR13</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR12</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR11</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR10</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR9</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR8</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x Reset bit y (y= 0 ..
              15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="GPIOB">
      <name>GPIOC</name>
      <baseAddress>0x50000800</baseAddress>
    </peripheral>
    <peripheral derivedFrom="GPIOB">
      <name>GPIOD</name>
      <baseAddress>0x50000C00</baseAddress>
    </peripheral>
    <peripheral derivedFrom="GPIOB">
      <name>GPIOH</name>
      <baseAddress>0x50001C00</baseAddress>
    </peripheral>
    <peripheral derivedFrom="GPIOB">
      <name>GPIOE</name>
      <baseAddress>0x50001000</baseAddress>
    </peripheral>
    <peripheral>
      <name>LCD</name>
      <description>Liquid crystal display controller</description>
      <groupName>LCD</groupName>
      <baseAddress>0x40002400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>LCD</name>
        <description>LCD global interrupt</description>
        <value>30</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BIAS</name>
              <description>Bias selector</description>
              <bitOffset>5</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DUTY</name>
              <description>Duty selection</description>
              <bitOffset>2</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>VSEL</name>
              <description>Voltage source selection</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCDEN</name>
              <description>LCD controller enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FCR</name>
          <displayName>FCR</displayName>
          <description>frame control register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PS</name>
              <description>PS 16-bit prescaler</description>
              <bitOffset>22</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>DIV</name>
              <description>DIV clock divider</description>
              <bitOffset>18</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>BLINK</name>
              <description>Blink mode selection</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>BLINKF</name>
              <description>Blink frequency selection</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>CC</name>
              <description>Contrast control</description>
              <bitOffset>10</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>DEAD</name>
              <description>Dead time duration</description>
              <bitOffset>7</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>PON</name>
              <description>Pulse ON duration</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>UDDIE</name>
              <description>Update display done interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SOFIE</name>
              <description>Start of frame interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HD</name>
              <description>High drive enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000020</resetValue>
          <fields>
            <field>
              <name>FCRSF</name>
              <description>LCD Frame Control Register
              Synchronization flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>RDY</name>
              <description>Ready flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>UDD</name>
              <description>Update Display Done</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>UDR</name>
              <description>Update display request</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>SOF</name>
              <description>Start of frame flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ENS</name>
              <description>ENS</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CLR</name>
          <displayName>CLR</displayName>
          <description>clear register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>UDDC</name>
              <description>Update display done clear</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SOFC</name>
              <description>Start of frame flag clear</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RAM_COM0</name>
          <displayName>RAM_COM0</displayName>
          <description>display memory</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>S30</name>
              <description>S30</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S29</name>
              <description>S29</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S28</name>
              <description>S28</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S27</name>
              <description>S27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S26</name>
              <description>S26</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S25</name>
              <description>S25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S24</name>
              <description>S24</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S23</name>
              <description>S23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S22</name>
              <description>S22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S21</name>
              <description>S21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S20</name>
              <description>S20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S19</name>
              <description>S19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S18</name>
              <description>S18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S17</name>
              <description>S17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S16</name>
              <description>S16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S15</name>
              <description>S15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S14</name>
              <description>S14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S13</name>
              <description>S13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S12</name>
              <description>S12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S11</name>
              <description>S11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S10</name>
              <description>S10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S09</name>
              <description>S09</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S08</name>
              <description>S08</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S07</name>
              <description>S07</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S06</name>
              <description>S06</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S05</name>
              <description>S05</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S04</name>
              <description>S04</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S03</name>
              <description>S03</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S02</name>
              <description>S02</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S01</name>
              <description>S01</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S00</name>
              <description>S00</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RAM_COM1</name>
          <displayName>RAM_COM1</displayName>
          <description>display memory</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>S31</name>
              <description>S31</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S30</name>
              <description>S30</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S29</name>
              <description>S29</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S28</name>
              <description>S28</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S27</name>
              <description>S27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S26</name>
              <description>S26</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S25</name>
              <description>S25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S24</name>
              <description>S24</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S23</name>
              <description>S23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S22</name>
              <description>S22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S21</name>
              <description>S21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S20</name>
              <description>S20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S19</name>
              <description>S19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S18</name>
              <description>S18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S17</name>
              <description>S17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S16</name>
              <description>S16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S15</name>
              <description>S15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S14</name>
              <description>S14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S13</name>
              <description>S13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S12</name>
              <description>S12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S11</name>
              <description>S11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S10</name>
              <description>S10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S09</name>
              <description>S09</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S08</name>
              <description>S08</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S07</name>
              <description>S07</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S06</name>
              <description>S06</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S05</name>
              <description>S05</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S04</name>
              <description>S04</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S03</name>
              <description>S03</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S02</name>
              <description>S02</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S01</name>
              <description>S01</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S00</name>
              <description>S00</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RAM_COM2</name>
          <displayName>RAM_COM2</displayName>
          <description>display memory</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>S31</name>
              <description>S31</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S30</name>
              <description>S30</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S29</name>
              <description>S29</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S28</name>
              <description>S28</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S27</name>
              <description>S27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S26</name>
              <description>S26</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S25</name>
              <description>S25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S24</name>
              <description>S24</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S23</name>
              <description>S23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S22</name>
              <description>S22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S21</name>
              <description>S21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S20</name>
              <description>S20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S19</name>
              <description>S19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S18</name>
              <description>S18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S17</name>
              <description>S17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S16</name>
              <description>S16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S15</name>
              <description>S15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S14</name>
              <description>S14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S13</name>
              <description>S13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S12</name>
              <description>S12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S11</name>
              <description>S11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S10</name>
              <description>S10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S09</name>
              <description>S09</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S08</name>
              <description>S08</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S07</name>
              <description>S07</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S06</name>
              <description>S06</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S05</name>
              <description>S05</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S04</name>
              <description>S04</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S03</name>
              <description>S03</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S02</name>
              <description>S02</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S01</name>
              <description>S01</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S00</name>
              <description>S00</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RAM_COM3</name>
          <displayName>RAM_COM3</displayName>
          <description>display memory</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>S31</name>
              <description>S31</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S30</name>
              <description>S30</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S29</name>
              <description>S29</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S28</name>
              <description>S28</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S27</name>
              <description>S27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S26</name>
              <description>S26</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S25</name>
              <description>S25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S24</name>
              <description>S24</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S23</name>
              <description>S23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S22</name>
              <description>S22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S21</name>
              <description>S21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S20</name>
              <description>S20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S19</name>
              <description>S19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S18</name>
              <description>S18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S17</name>
              <description>S17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S16</name>
              <description>S16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S15</name>
              <description>S15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S14</name>
              <description>S14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S13</name>
              <description>S13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S12</name>
              <description>S12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S11</name>
              <description>S11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S10</name>
              <description>S10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S09</name>
              <description>S09</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S08</name>
              <description>S08</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S07</name>
              <description>S07</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S06</name>
              <description>S06</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S05</name>
              <description>S05</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S04</name>
              <description>S04</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S03</name>
              <description>S03</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S02</name>
              <description>S02</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S01</name>
              <description>S01</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S00</name>
              <description>S00</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RAM_COM4</name>
          <displayName>RAM_COM4</displayName>
          <description>display memory</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>S31</name>
              <description>S31</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S30</name>
              <description>S30</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S29</name>
              <description>S29</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S28</name>
              <description>S28</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S27</name>
              <description>S27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S26</name>
              <description>S26</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S25</name>
              <description>S25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S24</name>
              <description>S24</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S23</name>
              <description>S23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S22</name>
              <description>S22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S21</name>
              <description>S21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S20</name>
              <description>S20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S19</name>
              <description>S19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S18</name>
              <description>S18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S17</name>
              <description>S17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S16</name>
              <description>S16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S15</name>
              <description>S15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S14</name>
              <description>S14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S13</name>
              <description>S13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S12</name>
              <description>S12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S11</name>
              <description>S11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S10</name>
              <description>S10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S09</name>
              <description>S09</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S08</name>
              <description>S08</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S07</name>
              <description>S07</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S06</name>
              <description>S06</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S05</name>
              <description>S05</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S04</name>
              <description>S04</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S03</name>
              <description>S03</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S02</name>
              <description>S02</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S01</name>
              <description>S01</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S00</name>
              <description>S00</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RAM_COM5</name>
          <displayName>RAM_COM5</displayName>
          <description>display memory</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>S31</name>
              <description>S31</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S30</name>
              <description>S30</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S29</name>
              <description>S29</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S28</name>
              <description>S28</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S27</name>
              <description>S27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S26</name>
              <description>S26</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S25</name>
              <description>S25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S24</name>
              <description>S24</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S23</name>
              <description>S23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S22</name>
              <description>S22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S21</name>
              <description>S21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S20</name>
              <description>S20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S19</name>
              <description>S19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S18</name>
              <description>S18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S17</name>
              <description>S17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S16</name>
              <description>S16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S15</name>
              <description>S15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S14</name>
              <description>S14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S13</name>
              <description>S13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S12</name>
              <description>S12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S11</name>
              <description>S11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S10</name>
              <description>S10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S09</name>
              <description>S09</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S08</name>
              <description>S08</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S07</name>
              <description>S07</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S06</name>
              <description>S06</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S05</name>
              <description>S05</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S04</name>
              <description>S04</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S03</name>
              <description>S03</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S02</name>
              <description>S02</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S01</name>
              <description>S01</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S00</name>
              <description>S00</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RAM_COM6</name>
          <displayName>RAM_COM6</displayName>
          <description>display memory</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>S31</name>
              <description>S31</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S30</name>
              <description>S30</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S29</name>
              <description>S29</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S28</name>
              <description>S28</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S27</name>
              <description>S27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S26</name>
              <description>S26</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S25</name>
              <description>S25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S24</name>
              <description>S24</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S23</name>
              <description>S23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S22</name>
              <description>S22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S21</name>
              <description>S21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S20</name>
              <description>S20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S19</name>
              <description>S19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S18</name>
              <description>S18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S17</name>
              <description>S17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S16</name>
              <description>S16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S15</name>
              <description>S15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S14</name>
              <description>S14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S13</name>
              <description>S13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S12</name>
              <description>S12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S11</name>
              <description>S11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S10</name>
              <description>S10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S09</name>
              <description>S09</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S08</name>
              <description>S08</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S07</name>
              <description>S07</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S06</name>
              <description>S06</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S05</name>
              <description>S05</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S04</name>
              <description>S04</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S03</name>
              <description>S03</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S02</name>
              <description>S02</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S01</name>
              <description>S01</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S00</name>
              <description>S00</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RAM_COM7</name>
          <displayName>RAM_COM7</displayName>
          <description>display memory</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>S31</name>
              <description>S31</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S30</name>
              <description>S30</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S29</name>
              <description>S29</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S28</name>
              <description>S28</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S27</name>
              <description>S27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S26</name>
              <description>S26</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S25</name>
              <description>S25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S24</name>
              <description>S24</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S23</name>
              <description>S23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S22</name>
              <description>S22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S21</name>
              <description>S21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S20</name>
              <description>S20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S19</name>
              <description>S19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S18</name>
              <description>S18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S17</name>
              <description>S17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S16</name>
              <description>S16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S15</name>
              <description>S15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S14</name>
              <description>S14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S13</name>
              <description>S13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S12</name>
              <description>S12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S11</name>
              <description>S11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S10</name>
              <description>S10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S09</name>
              <description>S09</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S08</name>
              <description>S08</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S07</name>
              <description>S07</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S06</name>
              <description>S06</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S05</name>
              <description>S05</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S04</name>
              <description>S04</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S03</name>
              <description>S03</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S02</name>
              <description>S02</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S01</name>
              <description>S01</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>S00</name>
              <description>S00</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>LPTIM</name>
      <description>Low power timer</description>
      <groupName>LPTIM</groupName>
      <baseAddress>0x40007C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>LPTIM1</name>
        <description>LPTIMER1 interrupt through
        EXTI29</description>
        <value>13</value>
      </interrupt>
      <registers>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>Interrupt and Status Register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DOWN</name>
              <description>Counter direction change up to
              down</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UP</name>
              <description>Counter direction change down to
              up</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARROK</name>
              <description>Autoreload register update
              OK</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPOK</name>
              <description>Compare register update OK</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTTRIG</name>
              <description>External trigger edge
              event</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARRM</name>
              <description>Autoreload match</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPM</name>
              <description>Compare match</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>Interrupt Clear Register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DOWNCF</name>
              <description>Direction change to down Clear
              Flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UPCF</name>
              <description>Direction change to UP Clear
              Flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARROKCF</name>
              <description>Autoreload register update OK Clear
              Flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPOKCF</name>
              <description>Compare register update OK Clear
              Flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTTRIGCF</name>
              <description>External trigger valid edge Clear
              Flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARRMCF</name>
              <description>Autoreload match Clear
              Flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPMCF</name>
              <description>compare match Clear Flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IER</name>
          <displayName>IER</displayName>
          <description>Interrupt Enable Register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DOWNIE</name>
              <description>Direction change to down Interrupt
              Enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UPIE</name>
              <description>Direction change to UP Interrupt
              Enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARROKIE</name>
              <description>Autoreload register update OK Interrupt
              Enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPOKIE</name>
              <description>Compare register update OK Interrupt
              Enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTTRIGIE</name>
              <description>External trigger valid edge Interrupt
              Enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARRMIE</name>
              <description>Autoreload match Interrupt
              Enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPMIE</name>
              <description>Compare match Interrupt
              Enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>Configuration Register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ENC</name>
              <description>Encoder mode enable</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>COUNTMODE</name>
              <description>counter mode enabled</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PRELOAD</name>
              <description>Registers update mode</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WAVPOL</name>
              <description>Waveform shape polarity</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WAVE</name>
              <description>Waveform shape</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIMOUT</name>
              <description>Timeout enable</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TRIGEN</name>
              <description>Trigger enable and
              polarity</description>
              <bitOffset>17</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TRIGSEL</name>
              <description>Trigger selector</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>PRESC</name>
              <description>Clock prescaler</description>
              <bitOffset>9</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TRGFLT</name>
              <description>Configurable digital filter for
              trigger</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CKFLT</name>
              <description>Configurable digital filter for external
              clock</description>
              <bitOffset>3</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CKPOL</name>
              <description>Clock Polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CKSEL</name>
              <description>Clock selector</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control Register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNTSTRT</name>
              <description>Timer start in continuous
              mode</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SNGSTRT</name>
              <description>LPTIM start in single mode</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ENABLE</name>
              <description>LPTIM Enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMP</name>
          <displayName>CMP</displayName>
          <description>Compare Register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CMP</name>
              <description>Compare value.</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>Autoreload Register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000001</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto reload value.</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>Counter Register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value.</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>RNG</name>
      <description>Random number generator</description>
      <groupName>RNG</groupName>
      <baseAddress>0x40025000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IE</name>
              <description>Interrupt enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RNGEN</name>
              <description>Random number generator
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SEIS</name>
              <description>Seed error interrupt
              status</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>CEIS</name>
              <description>Clock error interrupt
              status</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SECS</name>
              <description>Seed error current status</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>CECS</name>
              <description>Clock error current status</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DRDY</name>
              <description>Data ready</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>data register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>RNDATA</name>
              <description>Random data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>RTC</name>
      <description>Real-time clock</description>
      <groupName>RTC</groupName>
      <baseAddress>0x40002800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>RTC</name>
        <description>RTC global interrupt</description>
        <value>2</value>
      </interrupt>
      <registers>
        <register>
          <name>TR</name>
          <displayName>TR</displayName>
          <description>RTC time register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PM</name>
              <description>AM/PM notation</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HT</name>
              <description>Hour tens in BCD format</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>HU</name>
              <description>Hour units in BCD format</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MNT</name>
              <description>Minute tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MNU</name>
              <description>Minute units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ST</name>
              <description>Second tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SU</name>
              <description>Second units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>RTC date register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>YT</name>
              <description>Year tens in BCD format</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>YU</name>
              <description>Year units in BCD format</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>WDU</name>
              <description>Week day units</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MT</name>
              <description>Month tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MU</name>
              <description>Month units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>DT</name>
              <description>Date tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DU</name>
              <description>Date units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>RTC control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>COE</name>
              <description>Calibration output enable</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>OSEL</name>
              <description>Output selection</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>POL</name>
              <description>Output polarity</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COSEL</name>
              <description>Calibration output
              selection</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>BKP</name>
              <description>Backup</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SUB1H</name>
              <description>Subtract 1 hour (winter time
              change)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>ADD1H</name>
              <description>Add 1 hour (summer time
              change)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>TSIE</name>
              <description>Time-stamp interrupt
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>WUTIE</name>
              <description>Wakeup timer interrupt
              enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ALRBIE</name>
              <description>Alarm B interrupt enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ALRAIE</name>
              <description>Alarm A interrupt enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TSE</name>
              <description>timestamp enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>WUTE</name>
              <description>Wakeup timer enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ALRBE</name>
              <description>Alarm B enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ALRAE</name>
              <description>Alarm A enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FMT</name>
              <description>Hour format</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>BYPSHAD</name>
              <description>Bypass the shadow
              registers</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>REFCKON</name>
              <description>RTC_REFIN reference clock detection
              enable (50 or 60 Hz)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TSEDGE</name>
              <description>Time-stamp event active
              edge</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>WUCKSEL</name>
              <description>Wakeup clock selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>RTC initialization and status
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TAMP2F</name>
              <description>RTC_TAMP2 detection flag</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TAMP1F</name>
              <description>RTC_TAMP1 detection flag</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TSOVF</name>
              <description>Time-stamp overflow flag</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TSF</name>
              <description>Time-stamp flag</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>WUTF</name>
              <description>Wakeup timer flag</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ALRBF</name>
              <description>Alarm B flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ALRAF</name>
              <description>Alarm A flag</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>INIT</name>
              <description>Initialization mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>INITF</name>
              <description>Initialization flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>RSF</name>
              <description>Registers synchronization
              flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>INITS</name>
              <description>Initialization status flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SHPF</name>
              <description>Shift operation pending</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>WUTWF</name>
              <description>Wakeup timer write flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ALRBWF</name>
              <description>Alarm B write flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ALRAWF</name>
              <description>Alarm A write flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>PRER</name>
          <displayName>PRER</displayName>
          <description>RTC prescaler register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PREDIV_A</name>
              <description>Asynchronous prescaler
              factor</description>
              <bitOffset>16</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
            <field>
              <name>PREDIV_S</name>
              <description>Synchronous prescaler
              factor</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>WUTR</name>
          <displayName>WUTR</displayName>
          <description>RTC wakeup timer register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>WUT</name>
              <description>Wakeup auto-reload value
              bits</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ALRMAR</name>
          <displayName>ALRMAR</displayName>
          <description>RTC alarm A register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MSK4</name>
              <description>Alarm A date mask</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WDSEL</name>
              <description>Week day selection</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DT</name>
              <description>Date tens in BCD format.</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DU</name>
              <description>Date units or day in BCD
              format.</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK3</name>
              <description>Alarm A hours mask</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PM</name>
              <description>AM/PM notation</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HT</name>
              <description>Hour tens in BCD format.</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>HU</name>
              <description>Hour units in BCD format.</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK2</name>
              <description>Alarm A minutes mask</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MNT</name>
              <description>Minute tens in BCD format.</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MNU</name>
              <description>Minute units in BCD
              format.</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK1</name>
              <description>Alarm A seconds mask</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ST</name>
              <description>Second tens in BCD format.</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SU</name>
              <description>Second units in BCD
              format.</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ALRMBR</name>
          <displayName>ALRMBR</displayName>
          <description>RTC alarm B register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MSK4</name>
              <description>Alarm B date mask</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WDSEL</name>
              <description>Week day selection</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DT</name>
              <description>Date tens in BCD format</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DU</name>
              <description>Date units or day in BCD
              format</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK3</name>
              <description>Alarm B hours mask</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PM</name>
              <description>AM/PM notation</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HT</name>
              <description>Hour tens in BCD format</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>HU</name>
              <description>Hour units in BCD format</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK2</name>
              <description>Alarm B minutes mask</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MNT</name>
              <description>Minute tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MNU</name>
              <description>Minute units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK1</name>
              <description>Alarm B seconds mask</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ST</name>
              <description>Second tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SU</name>
              <description>Second units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>WPR</name>
          <displayName>WPR</displayName>
          <description>write protection register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>KEY</name>
              <description>Write protection key</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SSR</name>
          <displayName>SSR</displayName>
          <description>RTC sub second register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SS</name>
              <description>Sub second value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SHIFTR</name>
          <displayName>SHIFTR</displayName>
          <description>RTC shift control register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ADD1S</name>
              <description>Add one second</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SUBFS</name>
              <description>Subtract a fraction of a
              second</description>
              <bitOffset>0</bitOffset>
              <bitWidth>15</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TSTR</name>
          <displayName>TSTR</displayName>
          <description>RTC timestamp time register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PM</name>
              <description>AM/PM notation</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HT</name>
              <description>Hour tens in BCD format.</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>HU</name>
              <description>Hour units in BCD format.</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MNT</name>
              <description>Minute tens in BCD format.</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MNU</name>
              <description>Minute units in BCD
              format.</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ST</name>
              <description>Second tens in BCD format.</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SU</name>
              <description>Second units in BCD
              format.</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TSDR</name>
          <displayName>TSDR</displayName>
          <description>RTC timestamp date register</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>WDU</name>
              <description>Week day units</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MT</name>
              <description>Month tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MU</name>
              <description>Month units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>DT</name>
              <description>Date tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DU</name>
              <description>Date units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TSSSR</name>
          <displayName>TSSSR</displayName>
          <description>RTC time-stamp sub second
          register</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SS</name>
              <description>Sub second value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CALR</name>
          <displayName>CALR</displayName>
          <description>RTC calibration register</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CALP</name>
              <description>Use an 8-second calibration cycle
              period</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CALW8</name>
              <description>Use a 16-second calibration cycle
              period</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CALW16</name>
              <description>Reserved</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CALM</name>
              <description>Calibration minus</description>
              <bitOffset>0</bitOffset>
              <bitWidth>9</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TAMPCR</name>
          <displayName>TAMPCR</displayName>
          <description>RTC tamper configuration
          register</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TAMP2MF</name>
              <description>Tamper 2 mask flag</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP2NOERASE</name>
              <description>Tamper 2 no erase</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP2IE</name>
              <description>Tamper 2 interrupt enable</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP1MF</name>
              <description>Tamper 1 mask flag</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP1NOERASE</name>
              <description>Tamper 1 no erase</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP1IE</name>
              <description>Tamper 1 interrupt enable</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMPPUDIS</name>
              <description>RTC_TAMPx pull-up disable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMPPRCH</name>
              <description>RTC_TAMPx precharge
              duration</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TAMPFLT</name>
              <description>RTC_TAMPx filter count</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TAMPFREQ</name>
              <description>Tamper sampling frequency</description>
              <bitOffset>8</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TAMPTS</name>
              <description>Activate timestamp on tamper detection
              event</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP2_TRG</name>
              <description>Active level for RTC_TAMP2
              input</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP2E</name>
              <description>RTC_TAMP2 input detection
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMPIE</name>
              <description>Tamper interrupt enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP1TRG</name>
              <description>Active level for RTC_TAMP1
              input</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP1E</name>
              <description>RTC_TAMP1 input detection
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ALRMASSR</name>
          <displayName>ALRMASSR</displayName>
          <description>RTC alarm A sub second
          register</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MASKSS</name>
              <description>Mask the most-significant bits starting
              at this bit</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>SS</name>
              <description>Sub seconds value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>15</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ALRMBSSR</name>
          <displayName>ALRMBSSR</displayName>
          <description>RTC alarm B sub second
          register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MASKSS</name>
              <description>Mask the most-significant bits starting
              at this bit</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>SS</name>
              <description>Sub seconds value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>15</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OR</name>
          <displayName>OR</displayName>
          <description>option register</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>RTC_OUT_RMP</name>
              <description>RTC_ALARM on PC13 output
              type</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RTC_ALARM_TYPE</name>
              <description>RTC_ALARM on PC13 output
              type</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP0R</name>
          <displayName>BKP0R</displayName>
          <description>RTC backup registers</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP1R</name>
          <displayName>BKP1R</displayName>
          <description>RTC backup registers</description>
          <addressOffset>0x54</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP2R</name>
          <displayName>BKP2R</displayName>
          <description>RTC backup registers</description>
          <addressOffset>0x58</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP3R</name>
          <displayName>BKP3R</displayName>
          <description>RTC backup registers</description>
          <addressOffset>0x5C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP4R</name>
          <displayName>BKP4R</displayName>
          <description>RTC backup registers</description>
          <addressOffset>0x60</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>USART1</name>
      <description>Universal synchronous asynchronous receiver
      transmitter</description>
      <groupName>USART</groupName>
      <baseAddress>0x40013800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>USART1</name>
        <description>USART1 global interrupt</description>
        <value>27</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>M1</name>
              <description>Word length</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOBIE</name>
              <description>End of Block interrupt
              enable</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RTOIE</name>
              <description>Receiver timeout interrupt
              enable</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT4</name>
              <description>Driver Enable assertion
              time</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT3</name>
              <description>DEAT3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT2</name>
              <description>DEAT2</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT1</name>
              <description>DEAT1</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT0</name>
              <description>DEAT0</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT4</name>
              <description>Driver Enable de-assertion
              time</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT3</name>
              <description>DEDT3</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT2</name>
              <description>DEDT2</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT1</name>
              <description>DEDT1</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT0</name>
              <description>DEDT0</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVER8</name>
              <description>Oversampling mode</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMIE</name>
              <description>Character match interrupt
              enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MME</name>
              <description>Mute mode enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>M0</name>
              <description>Word length</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WAKE</name>
              <description>Receiver wakeup method</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PCE</name>
              <description>Parity control enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PS</name>
              <description>Parity selection</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PEIE</name>
              <description>PE interrupt enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXEIE</name>
              <description>interrupt enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transmission complete interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXNEIE</name>
              <description>RXNE interrupt enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDLEIE</name>
              <description>IDLE interrupt enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TE</name>
              <description>Transmitter enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RE</name>
              <description>Receiver enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UESM</name>
              <description>USART enable in Stop mode</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UE</name>
              <description>USART enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ADD4_7</name>
              <description>Address of the USART node</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ADD0_3</name>
              <description>Address of the USART node</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>RTOEN</name>
              <description>Receiver timeout enable</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ABRMOD1</name>
              <description>Auto baud rate mode</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ABRMOD0</name>
              <description>ABRMOD0</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ABREN</name>
              <description>Auto baud rate enable</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSBFIRST</name>
              <description>Most significant bit first</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAINV</name>
              <description>Binary data inversion</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXINV</name>
              <description>TX pin active level
              inversion</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXINV</name>
              <description>RX pin active level
              inversion</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWAP</name>
              <description>Swap TX/RX pins</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LINEN</name>
              <description>LIN mode enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOP</name>
              <description>STOP bits</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CLKEN</name>
              <description>Clock enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CPOL</name>
              <description>Clock polarity</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CPHA</name>
              <description>Clock phase</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LBCL</name>
              <description>Last bit clock pulse</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LBDIE</name>
              <description>LIN break detection interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LBDL</name>
              <description>LIN break detection length</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADDM7</name>
              <description>7-bit Address Detection/4-bit Address
              Detection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR3</name>
          <displayName>CR3</displayName>
          <description>Control register 3</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>WUFIE</name>
              <description>Wakeup from Stop mode interrupt
              enable</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WUS</name>
              <description>Wakeup from Stop mode interrupt flag
              selection</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SCARCNT</name>
              <description>Smartcard auto-retry count</description>
              <bitOffset>17</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>DEP</name>
              <description>Driver enable polarity
              selection</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEM</name>
              <description>Driver enable mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DDRE</name>
              <description>DMA Disable on Reception
              Error</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVRDIS</name>
              <description>Overrun Disable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ONEBIT</name>
              <description>One sample bit method
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSIE</name>
              <description>CTS interrupt enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSE</name>
              <description>CTS enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RTSE</name>
              <description>RTS enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAT</name>
              <description>DMA enable transmitter</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAR</name>
              <description>DMA enable receiver</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SCEN</name>
              <description>Smartcard mode enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NACK</name>
              <description>Smartcard NACK enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HDSEL</name>
              <description>Half-duplex selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IRLP</name>
              <description>Ir low-power</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IREN</name>
              <description>Ir mode enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EIE</name>
              <description>Error interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>Baud rate register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DIV_Mantissa</name>
              <description>DIV_Mantissa</description>
              <bitOffset>4</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>DIV_Fraction</name>
              <description>DIV_Fraction</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>GTPR</name>
          <displayName>GTPR</displayName>
          <description>Guard time and prescaler
          register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>GT</name>
              <description>Guard time value</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RTOR</name>
          <displayName>RTOR</displayName>
          <description>Receiver timeout register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>BLEN</name>
              <description>Block Length</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>RTO</name>
              <description>Receiver timeout value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>24</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RQR</name>
          <displayName>RQR</displayName>
          <description>Request register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TXFRQ</name>
              <description>Transmit data flush
              request</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXFRQ</name>
              <description>Receive data flush request</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MMRQ</name>
              <description>Mute mode request</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SBKRQ</name>
              <description>Send break request</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ABRRQ</name>
              <description>Auto baud rate request</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>Interrupt &amp; status
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00C0</resetValue>
          <fields>
            <field>
              <name>REACK</name>
              <description>REACK</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEACK</name>
              <description>TEACK</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WUF</name>
              <description>WUF</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RWU</name>
              <description>RWU</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SBKF</name>
              <description>SBKF</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMF</name>
              <description>CMF</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BUSY</name>
              <description>BUSY</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ABRF</name>
              <description>ABRF</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ABRE</name>
              <description>ABRE</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOBF</name>
              <description>EOBF</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RTOF</name>
              <description>RTOF</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTS</name>
              <description>CTS</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSIF</name>
              <description>CTSIF</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LBDF</name>
              <description>LBDF</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXE</name>
              <description>TXE</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TC</name>
              <description>TC</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXNE</name>
              <description>RXNE</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDLE</name>
              <description>IDLE</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ORE</name>
              <description>ORE</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NF</name>
              <description>NF</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FE</name>
              <description>FE</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PE</name>
              <description>PE</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>Interrupt flag clear register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>WUCF</name>
              <description>Wakeup from Stop mode clear
              flag</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMCF</name>
              <description>Character match clear flag</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOBCF</name>
              <description>End of block clear flag</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RTOCF</name>
              <description>Receiver timeout clear
              flag</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSCF</name>
              <description>CTS clear flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LBDCF</name>
              <description>LIN break detection clear
              flag</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCCF</name>
              <description>Transmission complete clear
              flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDLECF</name>
              <description>Idle line detected clear
              flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ORECF</name>
              <description>Overrun error clear flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NCF</name>
              <description>Noise detected clear flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FECF</name>
              <description>Framing error clear flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PECF</name>
              <description>Parity error clear flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RDR</name>
          <displayName>RDR</displayName>
          <description>Receive data register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>RDR</name>
              <description>Receive data value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>9</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TDR</name>
          <displayName>TDR</displayName>
          <description>Transmit data register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TDR</name>
              <description>Transmit data value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>9</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="USART1">
      <name>USART2</name>
      <baseAddress>0x40004400</baseAddress>
      <interrupt>
        <name>USART2</name>
        <description>USART2 global interrupt</description>
        <value>28</value>
      </interrupt>
    </peripheral>
    <peripheral derivedFrom="USART1">
      <name>USART4</name>
      <baseAddress>0x40004C00</baseAddress>
      <interrupt>
        <name>USART1</name>
        <description>USART1 global interrupt</description>
        <value>27</value>
      </interrupt>
    </peripheral>
    <peripheral derivedFrom="USART1">
      <name>USART5</name>
      <baseAddress>0x40005000</baseAddress>
      <interrupt>
        <name>USART2</name>
        <description>USART2 global interrupt</description>
        <value>28</value>
      </interrupt>
    </peripheral>
    <peripheral>
      <name>TSC</name>
      <description>Touch sensing controller</description>
      <groupName>TSC</groupName>
      <baseAddress>0x40024000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TSC</name>
        <description>Touch sensing interrupt</description>
        <value>8</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CTPH</name>
              <description>Charge transfer pulse high</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>CTPL</name>
              <description>Charge transfer pulse low</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>SSD</name>
              <description>Spread spectrum deviation</description>
              <bitOffset>17</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
            <field>
              <name>SSE</name>
              <description>Spread spectrum enable</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SSPSC</name>
              <description>Spread spectrum prescaler</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PGPSC</name>
              <description>pulse generator prescaler</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MCV</name>
              <description>Max count value</description>
              <bitOffset>5</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>IODEF</name>
              <description>I/O Default mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCPOL</name>
              <description>Synchronization pin
              polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AM</name>
              <description>Acquisition mode</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>START</name>
              <description>Start a new acquisition</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TSCE</name>
              <description>Touch sensing controller
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IER</name>
          <displayName>IER</displayName>
          <description>interrupt enable register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MCEIE</name>
              <description>Max count error interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOAIE</name>
              <description>End of acquisition interrupt
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>interrupt clear register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MCEIC</name>
              <description>Max count error interrupt
              clear</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOAIC</name>
              <description>End of acquisition interrupt
              clear</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>interrupt status register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MCEF</name>
              <description>Max count error flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOAF</name>
              <description>End of acquisition flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOHCR</name>
          <displayName>IOHCR</displayName>
          <description>I/O hysteresis control
          register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0xFFFFFFFF</resetValue>
          <fields>
            <field>
              <name>G8_IO4</name>
              <description>G8_IO4</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO3</name>
              <description>G8_IO3</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO2</name>
              <description>G8_IO2</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO1</name>
              <description>G8_IO1</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO4</name>
              <description>G7_IO4</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO3</name>
              <description>G7_IO3</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO2</name>
              <description>G7_IO2</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO1</name>
              <description>G7_IO1</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO4</name>
              <description>G6_IO4</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO3</name>
              <description>G6_IO3</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO2</name>
              <description>G6_IO2</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO1</name>
              <description>G6_IO1</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO4</name>
              <description>G5_IO4</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO3</name>
              <description>G5_IO3</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO2</name>
              <description>G5_IO2</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO1</name>
              <description>G5_IO1</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO4</name>
              <description>G4_IO4</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO3</name>
              <description>G4_IO3</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO2</name>
              <description>G4_IO2</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO1</name>
              <description>G4_IO1</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO4</name>
              <description>G3_IO4</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO3</name>
              <description>G3_IO3</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO2</name>
              <description>G3_IO2</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO1</name>
              <description>G3_IO1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO4</name>
              <description>G2_IO4</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO3</name>
              <description>G2_IO3</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO2</name>
              <description>G2_IO2</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO1</name>
              <description>G2_IO1</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO4</name>
              <description>G1_IO4</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO3</name>
              <description>G1_IO3</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO2</name>
              <description>G1_IO2</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO1</name>
              <description>G1_IO1</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOASCR</name>
          <displayName>IOASCR</displayName>
          <description>I/O analog switch control
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>G8_IO4</name>
              <description>G8_IO4</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO3</name>
              <description>G8_IO3</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO2</name>
              <description>G8_IO2</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO1</name>
              <description>G8_IO1</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO4</name>
              <description>G7_IO4</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO3</name>
              <description>G7_IO3</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO2</name>
              <description>G7_IO2</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO1</name>
              <description>G7_IO1</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO4</name>
              <description>G6_IO4</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO3</name>
              <description>G6_IO3</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO2</name>
              <description>G6_IO2</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO1</name>
              <description>G6_IO1</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO4</name>
              <description>G5_IO4</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO3</name>
              <description>G5_IO3</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO2</name>
              <description>G5_IO2</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO1</name>
              <description>G5_IO1</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO4</name>
              <description>G4_IO4</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO3</name>
              <description>G4_IO3</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO2</name>
              <description>G4_IO2</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO1</name>
              <description>G4_IO1</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO4</name>
              <description>G3_IO4</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO3</name>
              <description>G3_IO3</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO2</name>
              <description>G3_IO2</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO1</name>
              <description>G3_IO1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO4</name>
              <description>G2_IO4</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO3</name>
              <description>G2_IO3</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO2</name>
              <description>G2_IO2</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO1</name>
              <description>G2_IO1</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO4</name>
              <description>G1_IO4</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO3</name>
              <description>G1_IO3</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO2</name>
              <description>G1_IO2</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO1</name>
              <description>G1_IO1</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOSCR</name>
          <displayName>IOSCR</displayName>
          <description>I/O sampling control register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>G8_IO4</name>
              <description>G8_IO4</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO3</name>
              <description>G8_IO3</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO2</name>
              <description>G8_IO2</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO1</name>
              <description>G8_IO1</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO4</name>
              <description>G7_IO4</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO3</name>
              <description>G7_IO3</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO2</name>
              <description>G7_IO2</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO1</name>
              <description>G7_IO1</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO4</name>
              <description>G6_IO4</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO3</name>
              <description>G6_IO3</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO2</name>
              <description>G6_IO2</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO1</name>
              <description>G6_IO1</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO4</name>
              <description>G5_IO4</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO3</name>
              <description>G5_IO3</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO2</name>
              <description>G5_IO2</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO1</name>
              <description>G5_IO1</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO4</name>
              <description>G4_IO4</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO3</name>
              <description>G4_IO3</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO2</name>
              <description>G4_IO2</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO1</name>
              <description>G4_IO1</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO4</name>
              <description>G3_IO4</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO3</name>
              <description>G3_IO3</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO2</name>
              <description>G3_IO2</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO1</name>
              <description>G3_IO1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO4</name>
              <description>G2_IO4</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO3</name>
              <description>G2_IO3</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO2</name>
              <description>G2_IO2</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO1</name>
              <description>G2_IO1</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO4</name>
              <description>G1_IO4</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO3</name>
              <description>G1_IO3</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO2</name>
              <description>G1_IO2</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO1</name>
              <description>G1_IO1</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOCCR</name>
          <displayName>IOCCR</displayName>
          <description>I/O channel control register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>G8_IO4</name>
              <description>G8_IO4</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO3</name>
              <description>G8_IO3</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO2</name>
              <description>G8_IO2</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G8_IO1</name>
              <description>G8_IO1</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO4</name>
              <description>G7_IO4</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO3</name>
              <description>G7_IO3</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO2</name>
              <description>G7_IO2</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G7_IO1</name>
              <description>G7_IO1</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO4</name>
              <description>G6_IO4</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO3</name>
              <description>G6_IO3</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO2</name>
              <description>G6_IO2</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G6_IO1</name>
              <description>G6_IO1</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO4</name>
              <description>G5_IO4</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO3</name>
              <description>G5_IO3</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO2</name>
              <description>G5_IO2</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G5_IO1</name>
              <description>G5_IO1</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO4</name>
              <description>G4_IO4</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO3</name>
              <description>G4_IO3</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO2</name>
              <description>G4_IO2</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G4_IO1</name>
              <description>G4_IO1</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO4</name>
              <description>G3_IO4</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO3</name>
              <description>G3_IO3</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO2</name>
              <description>G3_IO2</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G3_IO1</name>
              <description>G3_IO1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO4</name>
              <description>G2_IO4</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO3</name>
              <description>G2_IO3</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO2</name>
              <description>G2_IO2</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G2_IO1</name>
              <description>G2_IO1</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO4</name>
              <description>G1_IO4</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO3</name>
              <description>G1_IO3</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO2</name>
              <description>G1_IO2</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>G1_IO1</name>
              <description>G1_IO1</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOGCSR</name>
          <displayName>IOGCSR</displayName>
          <description>I/O group control status
          register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>G8S</name>
              <description>Analog I/O group x status</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>G7S</name>
              <description>Analog I/O group x status</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>G6S</name>
              <description>Analog I/O group x status</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>G5S</name>
              <description>Analog I/O group x status</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>G4S</name>
              <description>Analog I/O group x status</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>G3S</name>
              <description>Analog I/O group x status</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>G2S</name>
              <description>Analog I/O group x status</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>G1S</name>
              <description>Analog I/O group x status</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>G8E</name>
              <description>Analog I/O group x enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>G7E</name>
              <description>Analog I/O group x enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>G6E</name>
              <description>Analog I/O group x enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>G5E</name>
              <description>Analog I/O group x enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>G4E</name>
              <description>Analog I/O group x enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>G3E</name>
              <description>Analog I/O group x enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>G2E</name>
              <description>Analog I/O group x enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>G1E</name>
              <description>Analog I/O group x enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>IOG1CR</name>
          <displayName>IOG1CR</displayName>
          <description>I/O group x counter register</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOG2CR</name>
          <displayName>IOG2CR</displayName>
          <description>I/O group x counter register</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOG3CR</name>
          <displayName>IOG3CR</displayName>
          <description>I/O group x counter register</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOG4CR</name>
          <displayName>IOG4CR</displayName>
          <description>I/O group x counter register</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOG5CR</name>
          <displayName>IOG5CR</displayName>
          <description>I/O group x counter register</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOG6CR</name>
          <displayName>IOG6CR</displayName>
          <description>I/O group x counter register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOG7CR</name>
          <displayName>IOG7CR</displayName>
          <description>I/O group x counter register</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOG8CR</name>
          <displayName>IOG8CR</displayName>
          <description>I/O group x counter register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>IWDG</name>
      <description>Independent watchdog</description>
      <groupName>IWDG</groupName>
      <baseAddress>0x40003000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>KR</name>
          <displayName>KR</displayName>
          <description>Key register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>KEY</name>
              <description>Key value (write only, read
              0x0000)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PR</name>
          <displayName>PR</displayName>
          <description>Prescaler register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PR</name>
              <description>Prescaler divider</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RLR</name>
          <displayName>RLR</displayName>
          <description>Reload register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000FFF</resetValue>
          <fields>
            <field>
              <name>RL</name>
              <description>Watchdog counter reload
              value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>WVU</name>
              <description>Watchdog counter window value
              update</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RVU</name>
              <description>Watchdog counter reload value
              update</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PVU</name>
              <description>Watchdog prescaler value
              update</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>WINR</name>
          <displayName>WINR</displayName>
          <description>Window register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000FFF</resetValue>
          <fields>
            <field>
              <name>WIN</name>
              <description>Watchdog counter window
              value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>WWDG</name>
      <description>System window watchdog</description>
      <groupName>WWDG</groupName>
      <baseAddress>0x40002C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>WWDG</name>
        <description>Window Watchdog interrupt</description>
        <value>0</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000007F</resetValue>
          <fields>
            <field>
              <name>WDGA</name>
              <description>Activation bit</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>T</name>
              <description>7-bit counter (MSB to LSB)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFR</name>
          <displayName>CFR</displayName>
          <description>Configuration register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000007F</resetValue>
          <fields>
            <field>
              <name>EWI</name>
              <description>Early wakeup interrupt</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WDGTB1</name>
              <description>Timer base</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WDGTB0</name>
              <description>WDGTB0</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>W</name>
              <description>7-bit window value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-writeOnce</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>EWIF</name>
              <description>Early wakeup interrupt
              flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>COMP</name>
      <description>Comparator</description>
      <groupName>COMP</groupName>
      <baseAddress>0x40010018</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x3E8</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>COMP1_CSR</name>
          <displayName>COMP1_CSR</displayName>
          <description>Comparator 1 control and status
          register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>COMP1_EN</name>
              <description>Comparator 1 enable bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP1_INN_SEL</name>
              <description>Comparator 1 Input Minus connection
              configuration bit</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP1_WM</name>
              <description>Comparator 1 window mode selection
              bit</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP1_OUT_SEL</name>
              <description>COMP1 output select</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP1_POLARITY</name>
              <description>Comparator 1 polarity selection
              bit</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP1_VALUE</name>
              <description>Comparator 1 output status
              bit</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>COMP1_LOCK</name>
              <description>COMP1_CSR register lock
              bit</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>COMP2_CSR</name>
          <displayName>COMP2_CSR</displayName>
          <description>Comparator 2 control and status
          register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>COMP2_LOCK</name>
              <description>COMP2_CSR register lock
              bit</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>COMP2_VALUE</name>
              <description>Comparator 2 output status
              bit</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>COMP2_POLARITY</name>
              <description>Comparator 2 polarity selection
              bit</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP2_INP_SEL</name>
              <description>Comparator 2 Input Plus connection
              configuration bit</description>
              <bitOffset>8</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP2_INN_SEL</name>
              <description>Comparator 2 Input Minus connection
              configuration bit</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP2_SPEED</name>
              <description>Comparator 2 power mode selection
              bit</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP2_EN</name>
              <description>Comparator 2 enable bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>COMP2_OUT_SEL</name>
              <description>COMP2 output select</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>USB_FS</name>
      <description>Universal serial bus full-speed device
      interface</description>
      <groupName>USB</groupName>
      <baseAddress>0x40005C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>USB</name>
        <description>USB event interrupt through
        EXTI18</description>
        <value>31</value>
      </interrupt>
      <registers>
        <register>
          <name>EP0R</name>
          <displayName>EP0R</displayName>
          <description>endpoint register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTR_RX</name>
              <description>CTR_RX</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_RX</name>
              <description>DTOG_RX</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_RX</name>
              <description>STAT_RX</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SETUP</name>
              <description>SETUP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EPTYPE</name>
              <description>EPTYPE</description>
              <bitOffset>9</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EP_KIND</name>
              <description>EP_KIND</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTR_TX</name>
              <description>CTR_TX</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_TX</name>
              <description>DTOG_TX</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_TX</name>
              <description>STAT_TX</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EA</name>
              <description>EA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EP1R</name>
          <displayName>EP1R</displayName>
          <description>endpoint register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTR_RX</name>
              <description>CTR_RX</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_RX</name>
              <description>DTOG_RX</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_RX</name>
              <description>STAT_RX</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SETUP</name>
              <description>SETUP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EPTYPE</name>
              <description>EPTYPE</description>
              <bitOffset>9</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EP_KIND</name>
              <description>EP_KIND</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTR_TX</name>
              <description>CTR_TX</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_TX</name>
              <description>DTOG_TX</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_TX</name>
              <description>STAT_TX</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EA</name>
              <description>EA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EP2R</name>
          <displayName>EP2R</displayName>
          <description>endpoint register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTR_RX</name>
              <description>CTR_RX</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_RX</name>
              <description>DTOG_RX</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_RX</name>
              <description>STAT_RX</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SETUP</name>
              <description>SETUP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EPTYPE</name>
              <description>EPTYPE</description>
              <bitOffset>9</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EP_KIND</name>
              <description>EP_KIND</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTR_TX</name>
              <description>CTR_TX</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_TX</name>
              <description>DTOG_TX</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_TX</name>
              <description>STAT_TX</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EA</name>
              <description>EA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EP3R</name>
          <displayName>EP3R</displayName>
          <description>endpoint register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTR_RX</name>
              <description>CTR_RX</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_RX</name>
              <description>DTOG_RX</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_RX</name>
              <description>STAT_RX</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SETUP</name>
              <description>SETUP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EPTYPE</name>
              <description>EPTYPE</description>
              <bitOffset>9</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EP_KIND</name>
              <description>EP_KIND</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTR_TX</name>
              <description>CTR_TX</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_TX</name>
              <description>DTOG_TX</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_TX</name>
              <description>STAT_TX</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EA</name>
              <description>EA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EP4R</name>
          <displayName>EP4R</displayName>
          <description>endpoint register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTR_RX</name>
              <description>CTR_RX</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_RX</name>
              <description>DTOG_RX</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_RX</name>
              <description>STAT_RX</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SETUP</name>
              <description>SETUP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EPTYPE</name>
              <description>EPTYPE</description>
              <bitOffset>9</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EP_KIND</name>
              <description>EP_KIND</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTR_TX</name>
              <description>CTR_TX</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_TX</name>
              <description>DTOG_TX</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_TX</name>
              <description>STAT_TX</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EA</name>
              <description>EA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EP5R</name>
          <displayName>EP5R</displayName>
          <description>endpoint register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTR_RX</name>
              <description>CTR_RX</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_RX</name>
              <description>DTOG_RX</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_RX</name>
              <description>STAT_RX</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SETUP</name>
              <description>SETUP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EPTYPE</name>
              <description>EPTYPE</description>
              <bitOffset>9</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EP_KIND</name>
              <description>EP_KIND</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTR_TX</name>
              <description>CTR_TX</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_TX</name>
              <description>DTOG_TX</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_TX</name>
              <description>STAT_TX</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EA</name>
              <description>EA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EP6R</name>
          <displayName>EP6R</displayName>
          <description>endpoint register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTR_RX</name>
              <description>CTR_RX</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_RX</name>
              <description>DTOG_RX</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_RX</name>
              <description>STAT_RX</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SETUP</name>
              <description>SETUP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EPTYPE</name>
              <description>EPTYPE</description>
              <bitOffset>9</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EP_KIND</name>
              <description>EP_KIND</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTR_TX</name>
              <description>CTR_TX</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_TX</name>
              <description>DTOG_TX</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_TX</name>
              <description>STAT_TX</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EA</name>
              <description>EA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EP7R</name>
          <displayName>EP7R</displayName>
          <description>endpoint register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTR_RX</name>
              <description>CTR_RX</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_RX</name>
              <description>DTOG_RX</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_RX</name>
              <description>STAT_RX</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SETUP</name>
              <description>SETUP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EPTYPE</name>
              <description>EPTYPE</description>
              <bitOffset>9</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EP_KIND</name>
              <description>EP_KIND</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTR_TX</name>
              <description>CTR_TX</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DTOG_TX</name>
              <description>DTOG_TX</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STAT_TX</name>
              <description>STAT_TX</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EA</name>
              <description>EA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNTR</name>
          <displayName>CNTR</displayName>
          <description>control register</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTRM</name>
              <description>CTRM</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PMAOVRM</name>
              <description>PMAOVRM</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRM</name>
              <description>ERRM</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WKUPM</name>
              <description>WKUPM</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SUSPM</name>
              <description>SUSPM</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RESETM</name>
              <description>RESETM</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SOFM</name>
              <description>SOFM</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ESOFM</name>
              <description>ESOFM</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>L1REQM</name>
              <description>L1REQM</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>L1RESUME</name>
              <description>L1RESUME</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RESUME</name>
              <description>RESUME</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FSUSP</name>
              <description>FSUSP</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPMODE</name>
              <description>LPMODE</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PDWN</name>
              <description>PDWN</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FRES</name>
              <description>FRES</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISTR</name>
          <displayName>ISTR</displayName>
          <description>interrupt status register</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>CTR</name>
              <description>CTR</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PMAOVR</name>
              <description>PMAOVR</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERR</name>
              <description>ERR</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WKUP</name>
              <description>WKUP</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SUSP</name>
              <description>SUSP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RESET</name>
              <description>RESET</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SOF</name>
              <description>SOF</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ESOF</name>
              <description>ESOF</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>L1REQ</name>
              <description>L1REQ</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>DIR</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EP_ID</name>
              <description>EP_ID</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FNR</name>
          <displayName>FNR</displayName>
          <description>frame number register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>RXDP</name>
              <description>RXDP</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXDM</name>
              <description>RXDM</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK</name>
              <description>LCK</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LSOF</name>
              <description>LSOF</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>FN</name>
              <description>FN</description>
              <bitOffset>0</bitOffset>
              <bitWidth>11</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DADDR</name>
          <displayName>DADDR</displayName>
          <description>device address</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>EF</name>
              <description>EF</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADD</name>
              <description>ADD</description>
              <bitOffset>0</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BTABLE</name>
          <displayName>BTABLE</displayName>
          <description>Buffer table address</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>BTABLE</name>
              <description>BTABLE</description>
              <bitOffset>3</bitOffset>
              <bitWidth>13</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>LPMCSR</name>
          <displayName>LPMCSR</displayName>
          <description>LPM control and status
          register</description>
          <addressOffset>0x54</addressOffset>
          <size>0x20</size>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>BESL</name>
              <description>BESL</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>REMWAKE</name>
              <description>REMWAKE</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>LPMACK</name>
              <description>LPMACK</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LPMEN</name>
              <description>LPMEN</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>BCDR</name>
          <displayName>BCDR</displayName>
          <description>Battery charging detector</description>
          <addressOffset>0x58</addressOffset>
          <size>0x20</size>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>DPPU</name>
              <description>DPPU</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PS2DET</name>
              <description>PS2DET</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SDET</name>
              <description>SDET</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>PDET</name>
              <description>PDET</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DCDET</name>
              <description>DCDET</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SDEN</name>
              <description>SDEN</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PDEN</name>
              <description>PDEN</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>DCDEN</name>
              <description>DCDEN</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>BCDEN</name>
              <description>BCDEN</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>CRS</name>
      <description>Clock recovery system</description>
      <groupName>CRS</groupName>
      <baseAddress>0x40006C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00002000</resetValue>
          <fields>
            <field>
              <name>TRIM</name>
              <description>HSI48 oscillator smooth
              trimming</description>
              <bitOffset>8</bitOffset>
              <bitWidth>6</bitWidth>
            </field>
            <field>
              <name>SWSYNC</name>
              <description>Generate software SYNC
              event</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AUTOTRIMEN</name>
              <description>Automatic trimming enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CEN</name>
              <description>Frequency error counter
              enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ESYNCIE</name>
              <description>Expected SYNC interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Synchronization or trimming error
              interrupt enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCWARNIE</name>
              <description>SYNC warning interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCOKIE</name>
              <description>SYNC event OK interrupt
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>configuration register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x2022BB7F</resetValue>
          <fields>
            <field>
              <name>SYNCPOL</name>
              <description>SYNC polarity selection</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCSRC</name>
              <description>SYNC signal source
              selection</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SYNCDIV</name>
              <description>SYNC divider</description>
              <bitOffset>24</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>FELIM</name>
              <description>Frequency error limit</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>RELOAD</name>
              <description>Counter reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>interrupt and status register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>FECAP</name>
              <description>Frequency error capture</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>FEDIR</name>
              <description>Frequency error direction</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TRIMOVF</name>
              <description>Trimming overflow or
              underflow</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCMISS</name>
              <description>SYNC missed</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCERR</name>
              <description>SYNC error</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ESYNCF</name>
              <description>Expected SYNC flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRF</name>
              <description>Error flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCWARNF</name>
              <description>SYNC warning flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCOKF</name>
              <description>SYNC event OK flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>interrupt flag clear register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ESYNCC</name>
              <description>Expected SYNC clear flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRC</name>
              <description>Error clear flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCWARNC</name>
              <description>SYNC warning clear flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYNCOKC</name>
              <description>SYNC event OK clear flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>Firewall</name>
      <description>Firewall</description>
      <groupName>Firewall</groupName>
      <baseAddress>0x40011C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>FIREWALL_CSSA</name>
          <displayName>FIREWALL_CSSA</displayName>
          <description>Code segment start address</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ADD</name>
              <description>code segment start address</description>
              <bitOffset>8</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FIREWALL_CSL</name>
          <displayName>FIREWALL_CSL</displayName>
          <description>Code segment length</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LENG</name>
              <description>code segment length</description>
              <bitOffset>8</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FIREWALL_NVDSSA</name>
          <displayName>FIREWALL_NVDSSA</displayName>
          <description>Non-volatile data segment start
          address</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ADD</name>
              <description>Non-volatile data segment start
              address</description>
              <bitOffset>8</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FIREWALL_NVDSL</name>
          <displayName>FIREWALL_NVDSL</displayName>
          <description>Non-volatile data segment
          length</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LENG</name>
              <description>Non-volatile data segment
              length</description>
              <bitOffset>8</bitOffset>
              <bitWidth>14</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FIREWALL_VDSSA</name>
          <displayName>FIREWALL_VDSSA</displayName>
          <description>Volatile data segment start
          address</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ADD</name>
              <description>Volatile data segment start
              address</description>
              <bitOffset>6</bitOffset>
              <bitWidth>10</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FIREWALL_VDSL</name>
          <displayName>FIREWALL_VDSL</displayName>
          <description>Volatile data segment length</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LENG</name>
              <description>Non-volatile data segment
              length</description>
              <bitOffset>6</bitOffset>
              <bitWidth>10</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FIREWALL_CR</name>
          <displayName>FIREWALL_CR</displayName>
          <description>Configuration register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>VDE</name>
              <description>Volatile data execution</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>VDS</name>
              <description>Volatile data shared</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FPA</name>
              <description>Firewall pre alarm</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>RCC</name>
      <description>Reset and clock control</description>
      <groupName>RCC</groupName>
      <baseAddress>0x40021000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>RCC</name>
        <description>RCC global interrupt</description>
        <value>4</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Clock control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000300</resetValue>
          <fields>
            <field>
              <name>PLLRDY</name>
              <description>PLL clock ready flag</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>PLLON</name>
              <description>PLL enable bit</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RTCPRE</name>
              <description>TC/LCD prescaler</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>CSSLSEON</name>
              <description>Clock security system on HSE enable
              bit</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSEBYP</name>
              <description>HSE clock bypass bit</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSERDY</name>
              <description>HSE clock ready flag</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSEON</name>
              <description>HSE clock enable bit</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MSIRDY</name>
              <description>MSI clock ready flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>MSION</name>
              <description>MSI clock enable bit</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSI16DIVF</name>
              <description>HSI16DIVF</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSI16DIVEN</name>
              <description>HSI16DIVEN</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSI16RDYF</name>
              <description>Internal high-speed clock ready
              flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSI16KERON</name>
              <description>High-speed internal clock enable bit for
              some IP kernels</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSI16ON</name>
              <description>16 MHz high-speed internal clock
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>ICSCR</name>
          <displayName>ICSCR</displayName>
          <description>Internal clock sources calibration
          register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <resetValue>0x0000B000</resetValue>
          <fields>
            <field>
              <name>MSITRIM</name>
              <description>MSI clock trimming</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MSICAL</name>
              <description>MSI clock calibration</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>MSIRANGE</name>
              <description>MSI clock ranges</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSI16TRIM</name>
              <description>High speed internal clock
              trimming</description>
              <bitOffset>8</bitOffset>
              <bitWidth>5</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSI16CAL</name>
              <description>nternal high speed clock
              calibration</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CRRCR</name>
          <displayName>CRRCR</displayName>
          <description>Clock recovery RC register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>HSI48CAL</name>
              <description>48 MHz HSI clock
              calibration</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSI48RDY</name>
              <description>48MHz HSI clock ready flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSI48ON</name>
              <description>48MHz HSI clock enable bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>Clock configuration register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MCOPRE</name>
              <description>Microcontroller clock output
              prescaler</description>
              <bitOffset>28</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MCOSEL</name>
              <description>Microcontroller clock output
              selection</description>
              <bitOffset>24</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PLLDIV</name>
              <description>PLL output division</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PLLMUL</name>
              <description>PLL multiplication factor</description>
              <bitOffset>18</bitOffset>
              <bitWidth>4</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PLLSRC</name>
              <description>PLL entry clock source</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>STOPWUCK</name>
              <description>Wake-up from stop clock
              selection</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PPRE2</name>
              <description>APB high-speed prescaler
              (APB2)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PPRE1</name>
              <description>APB low-speed prescaler
              (APB1)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HPRE</name>
              <description>AHB prescaler</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SWS</name>
              <description>System clock switch status</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SW</name>
              <description>System clock switch</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CIER</name>
          <displayName>CIER</displayName>
          <description>Clock interrupt enable
          register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CSSLSE</name>
              <description>LSE CSS interrupt flag</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HSI48RDYIE</name>
              <description>HSI48 ready interrupt flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIRDYIE</name>
              <description>MSI ready interrupt flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLRDYIE</name>
              <description>PLL ready interrupt flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HSERDYIE</name>
              <description>HSE ready interrupt flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HSI16RDYIE</name>
              <description>HSI16 ready interrupt flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LSERDYIE</name>
              <description>LSE ready interrupt flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LSIRDYIE</name>
              <description>LSI ready interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CIFR</name>
          <displayName>CIFR</displayName>
          <description>Clock interrupt flag register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CSSHSEF</name>
              <description>Clock Security System Interrupt
              flag</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CSSLSEF</name>
              <description>LSE Clock Security System Interrupt
              flag</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HSI48RDYF</name>
              <description>HSI48 ready interrupt flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIRDYF</name>
              <description>MSI ready interrupt flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLRDYF</name>
              <description>PLL ready interrupt flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HSERDYF</name>
              <description>HSE ready interrupt flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HSI16RDYF</name>
              <description>HSI16 ready interrupt flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LSERDYF</name>
              <description>LSE ready interrupt flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LSIRDYF</name>
              <description>LSI ready interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CICR</name>
          <displayName>CICR</displayName>
          <description>Clock interrupt clear register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CSSHSEC</name>
              <description>Clock Security System Interrupt
              clear</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CSSLSEC</name>
              <description>LSE Clock Security System Interrupt
              clear</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HSI48RDYC</name>
              <description>HSI48 ready Interrupt
              clear</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIRDYC</name>
              <description>MSI ready Interrupt clear</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLRDYC</name>
              <description>PLL ready Interrupt clear</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HSERDYC</name>
              <description>HSE ready Interrupt clear</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HSI16RDYC</name>
              <description>HSI16 ready Interrupt
              clear</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LSERDYC</name>
              <description>LSE ready Interrupt clear</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LSIRDYC</name>
              <description>LSI ready Interrupt clear</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOPRSTR</name>
          <displayName>IOPRSTR</displayName>
          <description>GPIO reset register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IOPHRST</name>
              <description>I/O port H reset</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPDRST</name>
              <description>I/O port D reset</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPCRST</name>
              <description>I/O port A reset</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPBRST</name>
              <description>I/O port B reset</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPARST</name>
              <description>I/O port A reset</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AHBRSTR</name>
          <displayName>AHBRSTR</displayName>
          <description>AHB peripheral reset register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CRYPRST</name>
              <description>Crypto module reset</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RNGRST</name>
              <description>Random Number Generator module
              reset</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TOUCHRST</name>
              <description>Touch Sensing reset</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCRST</name>
              <description>Test integration module
              reset</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MIFRST</name>
              <description>Memory interface reset</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMARST</name>
              <description>DMA reset</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB2RSTR</name>
          <displayName>APB2RSTR</displayName>
          <description>APB2 peripheral reset register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x000000000</resetValue>
          <fields>
            <field>
              <name>DBGRST</name>
              <description>DBG reset</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART1RST</name>
              <description>USART1 reset</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI1RST</name>
              <description>SPI 1 reset</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADCRST</name>
              <description>ADC interface reset</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TM12RST</name>
              <description>TIM22 timer reset</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM21RST</name>
              <description>TIM21 timer reset</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYSCFGRST</name>
              <description>System configuration controller
              reset</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB1RSTR</name>
          <displayName>APB1RSTR</displayName>
          <description>APB1 peripheral reset register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LPTIM1RST</name>
              <description>Low power timer reset</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DACRST</name>
              <description>DAC interface reset</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PWRRST</name>
              <description>Power interface reset</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRSRST</name>
              <description>Clock recovery system
              reset</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USBRST</name>
              <description>USB reset</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C2RST</name>
              <description>I2C2 reset</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C1RST</name>
              <description>I2C1 reset</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPUART1RST</name>
              <description>LPUART1 reset</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPUART12RST</name>
              <description>UART2 reset</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI2RST</name>
              <description>SPI2 reset</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WWDRST</name>
              <description>Window watchdog reset</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCDRST</name>
              <description>LCD reset</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM6RST</name>
              <description>Timer 6 reset</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM2RST</name>
              <description>Timer2 reset</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOPENR</name>
          <displayName>IOPENR</displayName>
          <description>GPIO clock enable register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IOPHEN</name>
              <description>I/O port H clock enable
              bit</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPDEN</name>
              <description>I/O port D clock enable
              bit</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPCEN</name>
              <description>IO port A clock enable bit</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPBEN</name>
              <description>IO port B clock enable bit</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPAEN</name>
              <description>IO port A clock enable bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AHBENR</name>
          <displayName>AHBENR</displayName>
          <description>AHB peripheral clock enable
          register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000100</resetValue>
          <fields>
            <field>
              <name>CRYPEN</name>
              <description>Crypto clock enable bit</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RNGEN</name>
              <description>Random Number Generator clock enable
              bit</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TOUCHEN</name>
              <description>Touch Sensing clock enable
              bit</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCEN</name>
              <description>CRC clock enable bit</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MIFEN</name>
              <description>NVM interface clock enable
              bit</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAEN</name>
              <description>DMA clock enable bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB2ENR</name>
          <displayName>APB2ENR</displayName>
          <description>APB2 peripheral clock enable
          register</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DBGEN</name>
              <description>DBG clock enable bit</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART1EN</name>
              <description>USART1 clock enable bit</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI1EN</name>
              <description>SPI1 clock enable bit</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADCEN</name>
              <description>ADC clock enable bit</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MIFIEN</name>
              <description>MiFaRe Firewall clock enable
              bit</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM22EN</name>
              <description>TIM22 timer clock enable
              bit</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM21EN</name>
              <description>TIM21 timer clock enable
              bit</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYSCFGEN</name>
              <description>System configuration controller clock
              enable bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB1ENR</name>
          <displayName>APB1ENR</displayName>
          <description>APB1 peripheral clock enable
          register</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LPTIM1EN</name>
              <description>Low power timer clock enable
              bit</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DACEN</name>
              <description>DAC interface clock enable
              bit</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PWREN</name>
              <description>Power interface clock enable
              bit</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRSEN</name>
              <description>Clock recovery system clock enable
              bit</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USBEN</name>
              <description>USB clock enable bit</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C2EN</name>
              <description>I2C2 clock enable bit</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C1EN</name>
              <description>I2C1 clock enable bit</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPUART1EN</name>
              <description>LPUART1 clock enable bit</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART2EN</name>
              <description>UART2 clock enable bit</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI2EN</name>
              <description>SPI2 clock enable bit</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WWDGEN</name>
              <description>Window watchdog clock enable
              bit</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCDEN</name>
              <description>LCD clock enable bit</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM6EN</name>
              <description>Timer 6 clock enable bit</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM2EN</name>
              <description>Timer2 clock enable bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IOPSMEN</name>
          <displayName>IOPSMEN</displayName>
          <description>GPIO clock enable in sleep mode
          register</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000008F</resetValue>
          <fields>
            <field>
              <name>IOPHSMEN</name>
              <description>IOPHSMEN</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPDSMEN</name>
              <description>IOPDSMEN</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPCSMEN</name>
              <description>IOPCSMEN</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPBSMEN</name>
              <description>IOPBSMEN</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IOPASMEN</name>
              <description>IOPASMEN</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AHBSMENR</name>
          <displayName>AHBSMENR</displayName>
          <description>AHB peripheral clock enable in sleep mode
          register</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x01111301</resetValue>
          <fields>
            <field>
              <name>CRYPSMEN</name>
              <description>Crypto clock enable during sleep mode
              bit</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RNGSMEN</name>
              <description>Random Number Generator clock enable
              during sleep mode bit</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TOUCHSMEN</name>
              <description>Touch Sensing clock enable during sleep
              mode bit</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCSMEN</name>
              <description>CRC clock enable during sleep mode
              bit</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SRAMSMEN</name>
              <description>SRAM interface clock enable during sleep
              mode bit</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MIFSMEN</name>
              <description>NVM interface clock enable during sleep
              mode bit</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMASMEN</name>
              <description>DMA clock enable during sleep mode
              bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB2SMENR</name>
          <displayName>APB2SMENR</displayName>
          <description>APB2 peripheral clock enable in sleep mode
          register</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00405225</resetValue>
          <fields>
            <field>
              <name>DBGSMEN</name>
              <description>DBG clock enable during sleep mode
              bit</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART1SMEN</name>
              <description>USART1 clock enable during sleep mode
              bit</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI1SMEN</name>
              <description>SPI1 clock enable during sleep mode
              bit</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADCSMEN</name>
              <description>ADC clock enable during sleep mode
              bit</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM22SMEN</name>
              <description>TIM22 timer clock enable during sleep
              mode bit</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM21SMEN</name>
              <description>TIM21 timer clock enable during sleep
              mode bit</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYSCFGSMEN</name>
              <description>System configuration controller clock
              enable during sleep mode bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB1SMENR</name>
          <displayName>APB1SMENR</displayName>
          <description>APB1 peripheral clock enable in sleep mode
          register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0xB8E64A11</resetValue>
          <fields>
            <field>
              <name>LPTIM1SMEN</name>
              <description>Low power timer clock enable during
              sleep mode bit</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DACSMEN</name>
              <description>DAC interface clock enable during sleep
              mode bit</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PWRSMEN</name>
              <description>Power interface clock enable during
              sleep mode bit</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRSSMEN</name>
              <description>Clock recovery system clock enable
              during sleep mode bit</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USBSMEN</name>
              <description>USB clock enable during sleep mode
              bit</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C2SMEN</name>
              <description>I2C2 clock enable during sleep mode
              bit</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C1SMEN</name>
              <description>I2C1 clock enable during sleep mode
              bit</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPUART1SMEN</name>
              <description>LPUART1 clock enable during sleep mode
              bit</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART2SMEN</name>
              <description>UART2 clock enable during sleep mode
              bit</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI2SMEN</name>
              <description>SPI2 clock enable during sleep mode
              bit</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WWDGSMEN</name>
              <description>Window watchdog clock enable during
              sleep mode bit</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCDSMEN</name>
              <description>LCD clock enable during sleep mode
              bit</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM6SMEN</name>
              <description>Timer 6 clock enable during sleep mode
              bit</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM2SMEN</name>
              <description>Timer2 clock enable during sleep mode
              bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCIPR</name>
          <displayName>CCIPR</displayName>
          <description>Clock configuration register</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>HSI48MSEL</name>
              <description>48 MHz HSI48 clock source selection
              bit</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPTIM1SEL1</name>
              <description>Low Power Timer clock source selection
              bits</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPTIM1SEL0</name>
              <description>LPTIM1SEL0</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C1SEL1</name>
              <description>I2C1 clock source selection
              bits</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C1SEL0</name>
              <description>I2C1SEL0</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPUART1SEL1</name>
              <description>LPUART1 clock source selection
              bits</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPUART1SEL0</name>
              <description>LPUART1SEL0</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART2SEL1</name>
              <description>USART2 clock source selection
              bits</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART2SEL0</name>
              <description>USART2SEL0</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART1SEL1</name>
              <description>USART1 clock source selection
              bits</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART1SEL0</name>
              <description>USART1SEL0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CSR</name>
          <displayName>CSR</displayName>
          <description>Control and status register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <resetValue>0x0C000000</resetValue>
          <fields>
            <field>
              <name>LPWRSTF</name>
              <description>Low-power reset flag</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>WWDGRSTF</name>
              <description>Window watchdog reset flag</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>IWDGRSTF</name>
              <description>Independent watchdog reset
              flag</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SFTRSTF</name>
              <description>Software reset flag</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PORRSTF</name>
              <description>POR/PDR reset flag</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PINRSTF</name>
              <description>PIN reset flag</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>OBLRSTF</name>
              <description>OBLRSTF</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RMVF</name>
              <description>Remove reset flag</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RTCRST</name>
              <description>RTC software reset bit</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RTCEN</name>
              <description>RTC clock enable bit</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RTCSEL</name>
              <description>RTC and LCD clock source selection
              bits</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>CSSLSED</name>
              <description>CSS on LSE failure detection
              flag</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>CSSLSEON</name>
              <description>CSSLSEON</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSEDRV</name>
              <description>LSEDRV</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSEBYP</name>
              <description>External low-speed oscillator bypass
              bit</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSERDY</name>
              <description>External low-speed oscillator ready
              bit</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>LSEON</name>
              <description>External low-speed oscillator enable
              bit</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSIRDY</name>
              <description>Internal low-speed oscillator ready
              bit</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSION</name>
              <description>Internal low-speed oscillator
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>SYSCFG</name>
      <description>System configuration controller</description>
      <groupName>SYSCFG</groupName>
      <baseAddress>0x40010000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CFGR1</name>
          <displayName>CFGR1</displayName>
          <description>SYSCFG configuration register
          1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BOOT_MODE</name>
              <description>Boot mode selected by the boot pins
              status bits</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>MEM_MODE</name>
              <description>Memory mapping selection
              bits</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR2</name>
          <displayName>CFGR2</displayName>
          <description>SYSCFG configuration register
          2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>I2C2_FMP</name>
              <description>I2C2 Fm+ drive capability enable
              bit</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C1_FMP</name>
              <description>I2C1 Fm+ drive capability enable
              bit</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C_PB9_FMP</name>
              <description>Fm+ drive capability on PB9 enable
              bit</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C_PB8_FMP</name>
              <description>Fm+ drive capability on PB8 enable
              bit</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C_PB7_FMP</name>
              <description>Fm+ drive capability on PB7 enable
              bit</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C_PB6_FMP</name>
              <description>Fm+ drive capability on PB6 enable
              bit</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CAPA</name>
              <description>Configuration of internal VLCD rail
              connection to optional external
              capacitor</description>
              <bitOffset>1</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>FWDISEN</name>
              <description>Firewall disable bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR1</name>
          <displayName>EXTICR1</displayName>
          <description>external interrupt configuration register
          1</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>EXTI3</name>
              <description>EXTI x configuration (x = 0 to
              3)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI2</name>
              <description>EXTI x configuration (x = 0 to
              3)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI1</name>
              <description>EXTI x configuration (x = 0 to
              3)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI0</name>
              <description>EXTI x configuration (x = 0 to
              3)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR2</name>
          <displayName>EXTICR2</displayName>
          <description>external interrupt configuration register
          2</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>EXTI7</name>
              <description>EXTI x configuration (x = 4 to
              7)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI6</name>
              <description>EXTI x configuration (x = 4 to
              7)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI5</name>
              <description>EXTI x configuration (x = 4 to
              7)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI4</name>
              <description>EXTI x configuration (x = 4 to
              7)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR3</name>
          <displayName>EXTICR3</displayName>
          <description>external interrupt configuration register
          3</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>EXTI11</name>
              <description>EXTI x configuration (x = 8 to
              11)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI10</name>
              <description>EXTI10</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI9</name>
              <description>EXTI x configuration (x = 8 to
              11)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI8</name>
              <description>EXTI x configuration (x = 8 to
              11)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR4</name>
          <displayName>EXTICR4</displayName>
          <description>external interrupt configuration register
          4</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>EXTI15</name>
              <description>EXTI x configuration (x = 12 to
              15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI14</name>
              <description>EXTI14</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI13</name>
              <description>EXTI13</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI12</name>
              <description>EXTI12</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR3</name>
          <displayName>CFGR3</displayName>
          <description>SYSCFG configuration register
          3</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>REF_LOCK</name>
              <description>REF_CTRL lock bit</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>VREFINT_RDYF</name>
              <description>VREFINT ready flag</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>VREFINT_COMP_RDYF</name>
              <description>VREFINT for comparator ready
              flag</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>VREFINT_ADC_RDYF</name>
              <description>VREFINT for ADC ready flag</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SENSOR_ADC_RDYF</name>
              <description>Sensor for ADC ready flag</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>REF_RC48MHz_RDYF</name>
              <description>VREFINT for 48 MHz RC oscillator ready
              flag</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ENREF_RC48MHz</name>
              <description>VREFINT reference for 48 MHz RC
              oscillator enable bit</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ENBUF_VREFINT_COMP</name>
              <description>VREFINT reference for comparator 2
              enable bit</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ENBUF_SENSOR_ADC</name>
              <description>Sensor reference for ADC enable
              bit</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ENBUF_BGAP_ADC</name>
              <description>VREFINT reference for ADC enable
              bit</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SEL_VREF_OUT</name>
              <description>BGAP_ADC connection bit</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>EN_BGAP</name>
              <description>Vref Enable bit</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>SPI1</name>
      <description>Serial peripheral interface</description>
      <groupName>SPI</groupName>
      <baseAddress>0x40013000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>SPI1</name>
        <description>SPI1_global_interrupt</description>
        <value>25</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>BIDIMODE</name>
              <description>Bidirectional data mode
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BIDIOE</name>
              <description>Output enable in bidirectional
              mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCEN</name>
              <description>Hardware CRC calculation
              enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCNEXT</name>
              <description>CRC transfer next</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DFF</name>
              <description>Data frame format</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXONLY</name>
              <description>Receive only</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SSM</name>
              <description>Software slave management</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SSI</name>
              <description>Internal slave select</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LSBFIRST</name>
              <description>Frame format</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPE</name>
              <description>SPI enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR</name>
              <description>Baud rate control</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MSTR</name>
              <description>Master selection</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CPOL</name>
              <description>Clock polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CPHA</name>
              <description>Clock phase</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>RXDMAEN</name>
              <description>Rx buffer DMA enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXDMAEN</name>
              <description>Tx buffer DMA enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SSOE</name>
              <description>SS output enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FRF</name>
              <description>Frame format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupt enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXNEIE</name>
              <description>RX buffer not empty interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXEIE</name>
              <description>Tx buffer empty interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <resetValue>0x0002</resetValue>
          <fields>
            <field>
              <name>RXNE</name>
              <description>Receive buffer not empty</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TXE</name>
              <description>Transmit buffer empty</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>CHSIDE</name>
              <description>Channel side</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>UDR</name>
              <description>Underrun flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>CRCERR</name>
              <description>CRC error flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MODF</name>
              <description>Mode fault</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>OVR</name>
              <description>Overrun flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>BSY</name>
              <description>Busy flag</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TIFRFE</name>
              <description>TI frame format error</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>data register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DR</name>
              <description>Data register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CRCPR</name>
          <displayName>CRCPR</displayName>
          <description>CRC polynomial register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0007</resetValue>
          <fields>
            <field>
              <name>CRCPOLY</name>
              <description>CRC polynomial register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RXCRCR</name>
          <displayName>RXCRCR</displayName>
          <description>RX CRC register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>RxCRC</name>
              <description>Rx CRC register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TXCRCR</name>
          <displayName>TXCRCR</displayName>
          <description>TX CRC register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TxCRC</name>
              <description>Tx CRC register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>I2SCFGR</name>
          <displayName>I2SCFGR</displayName>
          <description>I2S configuration register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>I2SMOD</name>
              <description>I2S mode selection</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2SE</name>
              <description>I2S Enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2SCFG</name>
              <description>I2S configuration mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PCMSYNC</name>
              <description>PCM frame synchronization</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2SSTD</name>
              <description>I2S standard selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CKPOL</name>
              <description>Steady state clock
              polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DATLEN</name>
              <description>Data length to be
              transferred</description>
              <bitOffset>1</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CHLEN</name>
              <description>Channel length (number of bits per audio
              channel)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>I2SPR</name>
          <displayName>I2SPR</displayName>
          <description>I2S prescaler register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000010</resetValue>
          <fields>
            <field>
              <name>MCKOE</name>
              <description>Master clock output enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODD</name>
              <description>Odd factor for the
              prescaler</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2SDIV</name>
              <description>I2S Linear prescaler</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="SPI1">
      <name>SPI2</name>
      <baseAddress>0x40003800</baseAddress>
      <interrupt>
        <name>SPI2</name>
        <description>SPI2 global interrupt</description>
        <value>26</value>
      </interrupt>
    </peripheral>
    <peripheral>
      <name>I2C1</name>
      <description>Inter-integrated circuit</description>
      <groupName>I2C</groupName>
      <baseAddress>0x40005400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>I2C1</name>
        <description>I2C1 global interrupt</description>
        <value>23</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PE</name>
              <description>Peripheral enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXIE</name>
              <description>TX Interrupt enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXIE</name>
              <description>RX Interrupt enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADDRIE</name>
              <description>Address match interrupt enable (slave
              only)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NACKIE</name>
              <description>Not acknowledge received interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOPIE</name>
              <description>STOP detection Interrupt
              enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer Complete interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupts enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DNF</name>
              <description>Digital noise filter</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ANFOFF</name>
              <description>Analog noise filter OFF</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXDMAEN</name>
              <description>DMA transmission requests
              enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXDMAEN</name>
              <description>DMA reception requests
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SBC</name>
              <description>Slave byte control</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NOSTRETCH</name>
              <description>Clock stretching disable</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WUPEN</name>
              <description>Wakeup from STOP enable</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GCEN</name>
              <description>General call enable</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SMBHEN</name>
              <description>SMBus Host address enable</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SMBDEN</name>
              <description>SMBus Device Default address
              enable</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ALERTEN</name>
              <description>SMBUS alert enable</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PECEN</name>
              <description>PEC enable</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PECBYTE</name>
              <description>Packet error checking byte</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AUTOEND</name>
              <description>Automatic end mode (master
              mode)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RELOAD</name>
              <description>NBYTES reload mode</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NBYTES</name>
              <description>Number of bytes</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>NACK</name>
              <description>NACK generation (slave
              mode)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOP</name>
              <description>Stop generation (master
              mode)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>START</name>
              <description>Start generation</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HEAD10R</name>
              <description>10-bit address header only read
              direction (master receiver mode)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADD10</name>
              <description>10-bit addressing mode (master
              mode)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RD_WRN</name>
              <description>Transfer direction (master
              mode)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SADD</name>
              <description>Slave address bit (master
              mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>10</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OAR1</name>
          <displayName>OAR1</displayName>
          <description>Own address register 1</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OA1</name>
              <description>Interface address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>10</bitWidth>
            </field>
            <field>
              <name>OA1MODE</name>
              <description>Own Address 1 10-bit mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OA1EN</name>
              <description>Own Address 1 enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OAR2</name>
          <displayName>OAR2</displayName>
          <description>Own address register 2</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OA2</name>
              <description>Interface address</description>
              <bitOffset>1</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
            <field>
              <name>OA2MSK</name>
              <description>Own Address 2 masks</description>
              <bitOffset>8</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OA2EN</name>
              <description>Own Address 2 enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TIMINGR</name>
          <displayName>TIMINGR</displayName>
          <description>Timing register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SCLL</name>
              <description>SCL low period (master
              mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>SCLH</name>
              <description>SCL high period (master
              mode)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>SDADEL</name>
              <description>Data hold time</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>SCLDEL</name>
              <description>Data setup time</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>PRESC</name>
              <description>Timing prescaler</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TIMEOUTR</name>
          <displayName>TIMEOUTR</displayName>
          <description>Status register 1</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TIMEOUTA</name>
              <description>Bus timeout A</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>TIDLE</name>
              <description>Idle clock timeout
              detection</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIMOUTEN</name>
              <description>Clock timeout enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIMEOUTB</name>
              <description>Bus timeout B</description>
              <bitOffset>16</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>TEXTEN</name>
              <description>Extended clock timeout
              enable</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>Interrupt and Status register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000001</resetValue>
          <fields>
            <field>
              <name>ADDCODE</name>
              <description>Address match code (Slave
              mode)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>7</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DIR</name>
              <description>Transfer direction (Slave
              mode)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>BUSY</name>
              <description>Bus busy</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ALERT</name>
              <description>SMBus alert</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TIMEOUT</name>
              <description>Timeout or t_low detection
              flag</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>PECERR</name>
              <description>PEC Error in reception</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>OVR</name>
              <description>Overrun/Underrun (slave
              mode)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ARLO</name>
              <description>Arbitration lost</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>BERR</name>
              <description>Bus error</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TCR</name>
              <description>Transfer Complete Reload</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TC</name>
              <description>Transfer Complete (master
              mode)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>STOPF</name>
              <description>Stop detection flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>NACKF</name>
              <description>Not acknowledge received
              flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ADDR</name>
              <description>Address matched (slave
              mode)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>RXNE</name>
              <description>Receive data register not empty
              (receivers)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TXIS</name>
              <description>Transmit interrupt status
              (transmitters)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TXE</name>
              <description>Transmit data register empty
              (transmitters)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>Interrupt clear register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ALERTCF</name>
              <description>Alert flag clear</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIMOUTCF</name>
              <description>Timeout detection flag
              clear</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PECCF</name>
              <description>PEC Error flag clear</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVRCF</name>
              <description>Overrun/Underrun flag
              clear</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARLOCF</name>
              <description>Arbitration lost flag
              clear</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BERRCF</name>
              <description>Bus error flag clear</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOPCF</name>
              <description>Stop detection flag clear</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NACKCF</name>
              <description>Not Acknowledge flag clear</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADDRCF</name>
              <description>Address Matched flag clear</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PECR</name>
          <displayName>PECR</displayName>
          <description>PEC register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PEC</name>
              <description>Packet error checking
              register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RXDR</name>
          <displayName>RXDR</displayName>
          <description>Receive data register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>RXDATA</name>
              <description>8-bit receive data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TXDR</name>
          <displayName>TXDR</displayName>
          <description>Transmit data register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TXDATA</name>
              <description>8-bit transmit data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="I2C1">
      <name>I2C2</name>
      <baseAddress>0x40005800</baseAddress>
      <interrupt>
        <name>I2C2</name>
        <description>I2C2 global interrupt</description>
        <value>24</value>
      </interrupt>
    </peripheral>
    <peripheral derivedFrom="I2C1">
      <name>I2C3</name>
      <baseAddress>0x40007800</baseAddress>
    </peripheral>
    <peripheral>
      <name>PWR</name>
      <description>Power control</description>
      <groupName>PWR</groupName>
      <baseAddress>0x40007000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>power control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00001000</resetValue>
          <fields>
            <field>
              <name>LPDS</name>
              <description>Low-power deep sleep</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PDDS</name>
              <description>Power down deepsleep</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CWUF</name>
              <description>Clear wakeup flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CSBF</name>
              <description>Clear standby flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PVDE</name>
              <description>Power voltage detector
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLS</name>
              <description>PVD level selection</description>
              <bitOffset>5</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>DBP</name>
              <description>Disable backup domain write
              protection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ULP</name>
              <description>Ultra-low-power mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FWU</name>
              <description>Fast wakeup</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>VOS</name>
              <description>Voltage scaling range
              selection</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DS_EE_KOFF</name>
              <description>Deep sleep mode with Flash memory kept
              off</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPRUN</name>
              <description>Low power run mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CSR</name>
          <displayName>CSR</displayName>
          <description>power control/status register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BRE</name>
              <description>Backup regulator enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>EWUP</name>
              <description>Enable WKUP pin</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>BRR</name>
              <description>Backup regulator ready</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>PVDO</name>
              <description>PVD output</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SBF</name>
              <description>Standby flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>WUF</name>
              <description>Wakeup flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>VOSF</name>
              <description>Voltage Scaling select
              flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>REGLPF</name>
              <description>Regulator LP flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>Flash</name>
      <description>Flash</description>
      <groupName>Flash</groupName>
      <baseAddress>0x40022000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>FLASH</name>
        <description>Flash global interrupt</description>
        <value>3</value>
      </interrupt>
      <registers>
        <register>
          <name>ACR</name>
          <displayName>ACR</displayName>
          <description>Access control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LATENCY</name>
              <description>Latency</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PRFTEN</name>
              <description>Prefetch enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SLEEP_PD</name>
              <description>Flash mode during Sleep</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RUN_PD</name>
              <description>Flash mode during Run</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DESAB_BUF</name>
              <description>Disable Buffer</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PRE_READ</name>
              <description>Pre-read data address</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PECR</name>
          <displayName>PECR</displayName>
          <description>Program/erase control register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000007</resetValue>
          <fields>
            <field>
              <name>PELOCK</name>
              <description>FLASH_PECR and data EEPROM
              lock</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PRGLOCK</name>
              <description>Program memory lock</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPTLOCK</name>
              <description>Option bytes block lock</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PROG</name>
              <description>Program memory selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DATA</name>
              <description>Data EEPROM selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FTDW</name>
              <description>Fixed time data write for Byte, Half
              Word and Word programming</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERASE</name>
              <description>Page or Double Word erase
              mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FPRG</name>
              <description>Half Page/Double Word programming
              mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PARALLELBANK</name>
              <description>Parallel bank mode</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOPIE</name>
              <description>End of programming interrupt
              enable</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupt enable</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OBL_LAUNCH</name>
              <description>Launch the option byte
              loading</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PDKEYR</name>
          <displayName>PDKEYR</displayName>
          <description>Power down key register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PDKEYR</name>
              <description>RUN_PD in FLASH_ACR key</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PEKEYR</name>
          <displayName>PEKEYR</displayName>
          <description>Program/erase key register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PEKEYR</name>
              <description>FLASH_PEC and data EEPROM
              key</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PRGKEYR</name>
          <displayName>PRGKEYR</displayName>
          <description>Program memory key register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRGKEYR</name>
              <description>Program memory key</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OPTKEYR</name>
          <displayName>OPTKEYR</displayName>
          <description>Option byte key register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OPTKEYR</name>
              <description>Option byte key</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000004</resetValue>
          <fields>
            <field>
              <name>BSY</name>
              <description>Write/erase operations in
              progress</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>EOP</name>
              <description>End of operation</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ENDHV</name>
              <description>End of high voltage</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>READY</name>
              <description>Flash memory module ready after low
              power mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>WRPERR</name>
              <description>Write protected error</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PGAERR</name>
              <description>Programming alignment
              error</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SIZERR</name>
              <description>Size error</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>OPTVERR</name>
              <description>Option validity error</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RDERR</name>
              <description>RDERR</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>NOTZEROERR</name>
              <description>NOTZEROERR</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FWWERR</name>
              <description>FWWERR</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>OBR</name>
          <displayName>OBR</displayName>
          <description>Option byte register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00F80000</resetValue>
          <fields>
            <field>
              <name>RDPRT</name>
              <description>Read protection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>BOR_LEV</name>
              <description>BOR_LEV</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>SPRMOD</name>
              <description>Selection of protection mode of WPR
              bits</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>WRPR</name>
          <displayName>WRPR</displayName>
          <description>Write protection register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>WRP</name>
              <description>Write protection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>EXTI</name>
      <description>External interrupt/event
      controller</description>
      <groupName>EXTI</groupName>
      <baseAddress>0x40010400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>PVD</name>
        <description>PVD through EXTI line detection</description>
        <value>1</value>
      </interrupt>
      <interrupt>
        <name>EXTI0_1</name>
        <description>EXTI Line[1:0] interrupts</description>
        <value>5</value>
      </interrupt>
      <interrupt>
        <name>EXTI2_3</name>
        <description>EXTI Line[3:2] interrupts</description>
        <value>6</value>
      </interrupt>
      <interrupt>
        <name>EXTI4_15</name>
        <description>EXTI Line15 and EXTI4 interrupts</description>
        <value>7</value>
      </interrupt>
      <registers>
        <register>
          <name>IMR</name>
          <displayName>IMR</displayName>
          <description>Interrupt mask register
          (EXTI_IMR)</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0xFF840000</resetValue>
          <fields>
            <field>
              <name>MR0</name>
              <description>Interrupt Mask on line 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR1</name>
              <description>Interrupt Mask on line 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR2</name>
              <description>Interrupt Mask on line 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR3</name>
              <description>Interrupt Mask on line 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR4</name>
              <description>Interrupt Mask on line 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR5</name>
              <description>Interrupt Mask on line 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR6</name>
              <description>Interrupt Mask on line 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR7</name>
              <description>Interrupt Mask on line 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR8</name>
              <description>Interrupt Mask on line 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR9</name>
              <description>Interrupt Mask on line 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR10</name>
              <description>Interrupt Mask on line 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR11</name>
              <description>Interrupt Mask on line 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR12</name>
              <description>Interrupt Mask on line 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR13</name>
              <description>Interrupt Mask on line 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR14</name>
              <description>Interrupt Mask on line 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR15</name>
              <description>Interrupt Mask on line 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR16</name>
              <description>Interrupt Mask on line 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR17</name>
              <description>Interrupt Mask on line 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR19</name>
              <description>Interrupt Mask on line 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR21</name>
              <description>Interrupt Mask on line 21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR22</name>
              <description>Interrupt Mask on line 22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR23</name>
              <description>Interrupt Mask on line 23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR25</name>
              <description>Interrupt Mask on line 25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR27</name>
              <description>Interrupt Mask on line 27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EMR</name>
          <displayName>EMR</displayName>
          <description>Event mask register (EXTI_EMR)</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MR0</name>
              <description>Event Mask on line 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR1</name>
              <description>Event Mask on line 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR2</name>
              <description>Event Mask on line 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR3</name>
              <description>Event Mask on line 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR4</name>
              <description>Event Mask on line 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR5</name>
              <description>Event Mask on line 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR6</name>
              <description>Event Mask on line 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR7</name>
              <description>Event Mask on line 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR8</name>
              <description>Event Mask on line 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR9</name>
              <description>Event Mask on line 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR10</name>
              <description>Event Mask on line 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR11</name>
              <description>Event Mask on line 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR12</name>
              <description>Event Mask on line 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR13</name>
              <description>Event Mask on line 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR14</name>
              <description>Event Mask on line 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR15</name>
              <description>Event Mask on line 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR16</name>
              <description>Event Mask on line 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR17</name>
              <description>Event Mask on line 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR19</name>
              <description>Event Mask on line 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR21</name>
              <description>Event Mask on line 21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR22</name>
              <description>Event Mask on line 22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR23</name>
              <description>Event Mask on line 23</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR25</name>
              <description>Event Mask on line 25</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR27</name>
              <description>Event Mask on line 27</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RTSR</name>
          <displayName>RTSR</displayName>
          <description>Rising Trigger selection register
          (EXTI_RTSR)</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TR0</name>
              <description>Rising trigger event configuration of
              line 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR1</name>
              <description>Rising trigger event configuration of
              line 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR2</name>
              <description>Rising trigger event configuration of
              line 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR3</name>
              <description>Rising trigger event configuration of
              line 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR4</name>
              <description>Rising trigger event configuration of
              line 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR5</name>
              <description>Rising trigger event configuration of
              line 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR6</name>
              <description>Rising trigger event configuration of
              line 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR7</name>
              <description>Rising trigger event configuration of
              line 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR8</name>
              <description>Rising trigger event configuration of
              line 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR9</name>
              <description>Rising trigger event configuration of
              line 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR10</name>
              <description>Rising trigger event configuration of
              line 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR11</name>
              <description>Rising trigger event configuration of
              line 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR12</name>
              <description>Rising trigger event configuration of
              line 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR13</name>
              <description>Rising trigger event configuration of
              line 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR14</name>
              <description>Rising trigger event configuration of
              line 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR15</name>
              <description>Rising trigger event configuration of
              line 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR16</name>
              <description>Rising trigger event configuration of
              line 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR17</name>
              <description>Rising trigger event configuration of
              line 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR19</name>
              <description>Rising trigger event configuration of
              line 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FTSR</name>
          <displayName>FTSR</displayName>
          <description>Falling Trigger selection register
          (EXTI_FTSR)</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TR0</name>
              <description>Falling trigger event configuration of
              line 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR1</name>
              <description>Falling trigger event configuration of
              line 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR2</name>
              <description>Falling trigger event configuration of
              line 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR3</name>
              <description>Falling trigger event configuration of
              line 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR4</name>
              <description>Falling trigger event configuration of
              line 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR5</name>
              <description>Falling trigger event configuration of
              line 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR6</name>
              <description>Falling trigger event configuration of
              line 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR7</name>
              <description>Falling trigger event configuration of
              line 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR8</name>
              <description>Falling trigger event configuration of
              line 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR9</name>
              <description>Falling trigger event configuration of
              line 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR10</name>
              <description>Falling trigger event configuration of
              line 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR11</name>
              <description>Falling trigger event configuration of
              line 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR12</name>
              <description>Falling trigger event configuration of
              line 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR13</name>
              <description>Falling trigger event configuration of
              line 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR14</name>
              <description>Falling trigger event configuration of
              line 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR15</name>
              <description>Falling trigger event configuration of
              line 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR16</name>
              <description>Falling trigger event configuration of
              line 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR17</name>
              <description>Falling trigger event configuration of
              line 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR19</name>
              <description>Falling trigger event configuration of
              line 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SWIER</name>
          <displayName>SWIER</displayName>
          <description>Software interrupt event register
          (EXTI_SWIER)</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SWIER0</name>
              <description>Software Interrupt on line
              0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER1</name>
              <description>Software Interrupt on line
              1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER2</name>
              <description>Software Interrupt on line
              2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER3</name>
              <description>Software Interrupt on line
              3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER4</name>
              <description>Software Interrupt on line
              4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER5</name>
              <description>Software Interrupt on line
              5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER6</name>
              <description>Software Interrupt on line
              6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER7</name>
              <description>Software Interrupt on line
              7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER8</name>
              <description>Software Interrupt on line
              8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER9</name>
              <description>Software Interrupt on line
              9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER10</name>
              <description>Software Interrupt on line
              10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER11</name>
              <description>Software Interrupt on line
              11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER12</name>
              <description>Software Interrupt on line
              12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER13</name>
              <description>Software Interrupt on line
              13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER14</name>
              <description>Software Interrupt on line
              14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER15</name>
              <description>Software Interrupt on line
              15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER16</name>
              <description>Software Interrupt on line
              16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER17</name>
              <description>Software Interrupt on line
              17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER19</name>
              <description>Software Interrupt on line
              19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PR</name>
          <displayName>PR</displayName>
          <description>Pending register (EXTI_PR)</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PR0</name>
              <description>Pending bit 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR1</name>
              <description>Pending bit 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR2</name>
              <description>Pending bit 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR3</name>
              <description>Pending bit 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR4</name>
              <description>Pending bit 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR5</name>
              <description>Pending bit 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR6</name>
              <description>Pending bit 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR7</name>
              <description>Pending bit 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR8</name>
              <description>Pending bit 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR9</name>
              <description>Pending bit 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR10</name>
              <description>Pending bit 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR11</name>
              <description>Pending bit 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR12</name>
              <description>Pending bit 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR13</name>
              <description>Pending bit 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR14</name>
              <description>Pending bit 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR15</name>
              <description>Pending bit 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR16</name>
              <description>Pending bit 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR17</name>
              <description>Pending bit 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR19</name>
              <description>Pending bit 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>ADC</name>
      <description>Analog-to-digital converter</description>
      <groupName>ADC</groupName>
      <baseAddress>0x40012400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>ADC_COMP</name>
        <description>ADC and comparator 1 and 2</description>
        <value>12</value>
      </interrupt>
      <registers>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>interrupt and status register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ADRDY</name>
              <description>ADC ready</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOSMP</name>
              <description>End of sampling flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOC</name>
              <description>End of conversion flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOS</name>
              <description>End of sequence flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVR</name>
              <description>ADC overrun</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWD</name>
              <description>Analog watchdog flag</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOCAL</name>
              <description>End Of Calibration flag</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IER</name>
          <displayName>IER</displayName>
          <description>interrupt enable register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ADRDYIE</name>
              <description>ADC ready interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOSMPIE</name>
              <description>End of sampling flag interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOCIE</name>
              <description>End of conversion interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOSIE</name>
              <description>End of conversion sequence interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVRIE</name>
              <description>Overrun interrupt enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWDIE</name>
              <description>Analog watchdog interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOCALIE</name>
              <description>End of calibration interrupt
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ADEN</name>
              <description>ADC enable command</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADDIS</name>
              <description>ADC disable command</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADSTART</name>
              <description>ADC start conversion
              command</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADSTP</name>
              <description>ADC stop conversion
              command</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADVREGEN</name>
              <description>ADC Voltage Regulator
              Enable</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADCAL</name>
              <description>ADC calibration</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR1</name>
          <displayName>CFGR1</displayName>
          <description>configuration register 1</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AWDCH</name>
              <description>Analog watchdog channel
              selection</description>
              <bitOffset>26</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>AWDEN</name>
              <description>Analog watchdog enable</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWDSGL</name>
              <description>Enable the watchdog on a single channel
              or on all channels</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DISCEN</name>
              <description>Discontinuous mode</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AUTOFF</name>
              <description>Auto-off mode</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AUTDLY</name>
              <description>Auto-delayed conversion
              mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CONT</name>
              <description>Single / continuous conversion
              mode</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVRMOD</name>
              <description>Overrun management mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTEN</name>
              <description>External trigger enable and polarity
              selection</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EXTSEL</name>
              <description>External trigger selection</description>
              <bitOffset>6</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>ALIGN</name>
              <description>Data alignment</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RES</name>
              <description>Data resolution</description>
              <bitOffset>3</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>SCANDIR</name>
              <description>Scan sequence direction</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMACFG</name>
              <description>Direct memery access
              configuration</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAEN</name>
              <description>Direct memory access
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR2</name>
          <displayName>CFGR2</displayName>
          <description>configuration register 2</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OVSE</name>
              <description>Oversampler Enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVSR</name>
              <description>Oversampling ratio</description>
              <bitOffset>2</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OVSS</name>
              <description>Oversampling shift</description>
              <bitOffset>5</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>TOVS</name>
              <description>Triggered Oversampling</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CKMODE</name>
              <description>ADC clock mode</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SMPR</name>
          <displayName>SMPR</displayName>
          <description>sampling time register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SMPR</name>
              <description>Sampling time selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TR</name>
          <displayName>TR</displayName>
          <description>watchdog threshold register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0FFF0000</resetValue>
          <fields>
            <field>
              <name>HT</name>
              <description>Analog watchdog higher
              threshold</description>
              <bitOffset>16</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>LT</name>
              <description>Analog watchdog lower
              threshold</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CHSELR</name>
          <displayName>CHSELR</displayName>
          <description>channel selection register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CHSEL18</name>
              <description>Channel-x selection</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL17</name>
              <description>Channel-x selection</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL16</name>
              <description>Channel-x selection</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL15</name>
              <description>Channel-x selection</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL14</name>
              <description>Channel-x selection</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL13</name>
              <description>Channel-x selection</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL12</name>
              <description>Channel-x selection</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL11</name>
              <description>Channel-x selection</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL10</name>
              <description>Channel-x selection</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL9</name>
              <description>Channel-x selection</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL8</name>
              <description>Channel-x selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL7</name>
              <description>Channel-x selection</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL6</name>
              <description>Channel-x selection</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL5</name>
              <description>Channel-x selection</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL4</name>
              <description>Channel-x selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL3</name>
              <description>Channel-x selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL2</name>
              <description>Channel-x selection</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL1</name>
              <description>Channel-x selection</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHSEL0</name>
              <description>Channel-x selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>data register</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DATA</name>
              <description>Converted data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CALFACT</name>
          <displayName>CALFACT</displayName>
          <description>ADC Calibration factor</description>
          <addressOffset>0xB4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CALFACT</name>
              <description>Calibration factor</description>
              <bitOffset>0</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR</name>
          <displayName>CCR</displayName>
          <description>ADC common configuration
          register</description>
          <addressOffset>0x308</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRESC</name>
              <description>ADC prescaler</description>
              <bitOffset>18</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>VREFEN</name>
              <description>VREFINT enable</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TSEN</name>
              <description>Temperature sensor enable</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>VLCDEN</name>
              <description>VLCD enable</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LFMEN</name>
              <description>Low Frequency Mode enable</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>DBGMCU</name>
      <description>Debug support</description>
      <groupName>DBGMCU</groupName>
      <baseAddress>0x40015800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>IDCODE</name>
          <displayName>IDCODE</displayName>
          <description>MCU Device ID Code Register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>DEV_ID</name>
              <description>Device Identifier</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>REV_ID</name>
              <description>Revision Identifier</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Debug MCU Configuration
          Register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>DBG_STOP</name>
              <description>Debug Stop Mode</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_STANDBY</name>
              <description>Debug Standby Mode</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_SLEEP</name>
              <description>Debug Sleep Mode</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB1_FZ</name>
          <displayName>APB1_FZ</displayName>
          <description>APB Low Freeze Register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>DBG_TIMER2_STOP</name>
              <description>Debug Timer 2 stopped when Core is
              halted</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_TIMER6_STOP</name>
              <description>Debug Timer 6 stopped when Core is
              halted</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_RTC_STOP</name>
              <description>Debug RTC stopped when Core is
              halted</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_WWDG_STOP</name>
              <description>Debug Window Wachdog stopped when Core
              is halted</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_IWDG_STOP</name>
              <description>Debug Independent Wachdog stopped when
              Core is halted</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_I2C1_STOP</name>
              <description>I2C1 SMBUS timeout mode stopped when
              core is halted</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_I2C2_STOP</name>
              <description>I2C2 SMBUS timeout mode stopped when
              core is halted</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_LPTIMER_STOP</name>
              <description>LPTIM1 counter stopped when core is
              halted</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB2_FZ</name>
          <displayName>APB2_FZ</displayName>
          <description>APB High Freeze Register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0</resetValue>
          <fields>
            <field>
              <name>DBG_TIMER21_STOP</name>
              <description>Debug Timer 21 stopped when Core is
              halted</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_TIMER22_STO</name>
              <description>Debug Timer 22 stopped when Core is
              halted</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM2</name>
      <description>General-purpose-timers</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40000000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM2</name>
        <description>TIM2 global interrupt</description>
        <value>15</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CKD</name>
              <description>Clock division</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMS</name>
              <description>Center-aligned mode
              selection</description>
              <bitOffset>5</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPM</name>
              <description>One-pulse mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TI1S</name>
              <description>TI1 selection</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MMS</name>
              <description>Master mode selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>CCDS</name>
              <description>Capture/compare DMA
              selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SMCR</name>
          <displayName>SMCR</displayName>
          <description>slave mode control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ETP</name>
              <description>External trigger polarity</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ECE</name>
              <description>External clock enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ETPS</name>
              <description>External trigger prescaler</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ETF</name>
              <description>External trigger filter</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSM</name>
              <description>Master/Slave mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TS</name>
              <description>Trigger selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SMS</name>
              <description>Slave mode selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TDE</name>
              <description>Trigger DMA request enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>COMDE</name>
              <description>Reserved</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4DE</name>
              <description>Capture/Compare 4 DMA request
              enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3DE</name>
              <description>Capture/Compare 3 DMA request
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2DE</name>
              <description>Capture/Compare 2 DMA request
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1DE</name>
              <description>Capture/Compare 1 DMA request
              enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDE</name>
              <description>Update DMA request enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIE</name>
              <description>Trigger interrupt enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4IE</name>
              <description>Capture/Compare 4 interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3IE</name>
              <description>Capture/Compare 3 interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IE</name>
              <description>Capture/Compare 2 interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IE</name>
              <description>Capture/Compare 1 interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC4OF</name>
              <description>Capture/Compare 4 overcapture
              flag</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3OF</name>
              <description>Capture/Compare 3 overcapture
              flag</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2OF</name>
              <description>Capture/compare 2 overcapture
              flag</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1OF</name>
              <description>Capture/Compare 1 overcapture
              flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIF</name>
              <description>Trigger interrupt flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4IF</name>
              <description>Capture/Compare 4 interrupt
              flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3IF</name>
              <description>Capture/Compare 3 interrupt
              flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IF</name>
              <description>Capture/Compare 2 interrupt
              flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IF</name>
              <description>Capture/compare 1 interrupt
              flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TG</name>
              <description>Trigger generation</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4G</name>
              <description>Capture/compare 4
              generation</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3G</name>
              <description>Capture/compare 3
              generation</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2G</name>
              <description>Capture/compare 2
              generation</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1G</name>
              <description>Capture/compare 1
              generation</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Output</name>
          <displayName>CCMR1_Output</displayName>
          <description>capture/compare mode register 1 (output
          mode)</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OC2CE</name>
              <description>Output compare 2 clear
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC2M</name>
              <description>Output compare 2 mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC2PE</name>
              <description>Output compare 2 preload
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC2FE</name>
              <description>Output compare 2 fast
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OC1CE</name>
              <description>Output compare 1 clear
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1M</name>
              <description>Output compare 1 mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC1PE</name>
              <description>Output compare 1 preload
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1FE</name>
              <description>Output compare 1 fast
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Input</name>
          <displayName>CCMR1_Input</displayName>
          <description>capture/compare mode register 1 (input
          mode)</description>
          <alternateRegister>CCMR1_Output</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC2F</name>
              <description>Input capture 2 filter</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC2PSC</name>
              <description>Input capture 2 prescaler</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>IC1F</name>
              <description>Input capture 1 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC1PSC</name>
              <description>Input capture 1 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_Output</name>
          <displayName>CCMR2_Output</displayName>
          <description>capture/compare mode register 2 (output
          mode)</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OC4CE</name>
              <description>Output compare 4 clear
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC4M</name>
              <description>Output compare 4 mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC4PE</name>
              <description>Output compare 4 preload
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC4FE</name>
              <description>Output compare 4 fast
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4S</name>
              <description>Capture/Compare 4
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OC3CE</name>
              <description>Output compare 3 clear
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC3M</name>
              <description>Output compare 3 mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC3PE</name>
              <description>Output compare 3 preload
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC3FE</name>
              <description>Output compare 3 fast
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3S</name>
              <description>Capture/Compare 3
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_Input</name>
          <displayName>CCMR2_Input</displayName>
          <description>capture/compare mode register 2 (input
          mode)</description>
          <alternateRegister>CCMR2_Output</alternateRegister>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC4F</name>
              <description>Input capture 4 filter</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC4PSC</name>
              <description>Input capture 4 prescaler</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC4S</name>
              <description>Capture/Compare 4
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>IC3F</name>
              <description>Input capture 3 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC3PSC</name>
              <description>Input capture 3 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC3S</name>
              <description>Capture/Compare 3
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <displayName>CCER</displayName>
          <description>capture/compare enable
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC4NP</name>
              <description>Capture/Compare 4 output
              Polarity</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4P</name>
              <description>Capture/Compare 3 output
              Polarity</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4E</name>
              <description>Capture/Compare 4 output
              enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3NP</name>
              <description>Capture/Compare 3 output
              Polarity</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3P</name>
              <description>Capture/Compare 3 output
              Polarity</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3E</name>
              <description>Capture/Compare 3 output
              enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2NP</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2P</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2E</name>
              <description>Capture/Compare 2 output
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1NP</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1P</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1E</name>
              <description>Capture/Compare 1 output
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT_H</name>
              <description>High counter value (TIM2
              only)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CNT_L</name>
              <description>Low counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ARR_H</name>
              <description>High Auto-reload value (TIM2
              only)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>ARR_L</name>
              <description>Low Auto-reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <displayName>CCR1</displayName>
          <description>capture/compare register 1</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR1_H</name>
              <description>High Capture/Compare 1 value (TIM2
              only)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CCR1_L</name>
              <description>Low Capture/Compare 1
              value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR2</name>
          <displayName>CCR2</displayName>
          <description>capture/compare register 2</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR2_H</name>
              <description>High Capture/Compare 2 value (TIM2
              only)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CCR2_L</name>
              <description>Low Capture/Compare 2
              value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR3</name>
          <displayName>CCR3</displayName>
          <description>capture/compare register 3</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR3_H</name>
              <description>High Capture/Compare value (TIM2
              only)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CCR3_L</name>
              <description>Low Capture/Compare value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR4</name>
          <displayName>CCR4</displayName>
          <description>capture/compare register 4</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR4_H</name>
              <description>High Capture/Compare value (TIM2
              only)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CCR4_L</name>
              <description>Low Capture/Compare value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DCR</name>
          <displayName>DCR</displayName>
          <description>DMA control register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DBL</name>
              <description>DMA burst length</description>
              <bitOffset>8</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>DBA</name>
              <description>DMA base address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DMAR</name>
          <displayName>DMAR</displayName>
          <description>DMA address for full transfer</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DMAB</name>
              <description>DMA register for burst
              accesses</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OR</name>
          <displayName>OR</displayName>
          <description>TIM2 option register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ETR_RMP</name>
              <description>Timer2 ETR remap</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TI4_RMP</name>
              <description>Internal trigger</description>
              <bitOffset>3</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="TIM2">
      <name>TIM3</name>
      <baseAddress>0x40000400</baseAddress>
      <interrupt>
        <name>TIM2</name>
        <description>TIM2 global interrupt</description>
        <value>15</value>
      </interrupt>
    </peripheral>
    <peripheral>
      <name>TIM6</name>
      <description>Basic-timers</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40001000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM6_DAC</name>
        <description>TIM6 global interrupt and DAC</description>
        <value>17</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPM</name>
              <description>One-pulse mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>MMS</name>
              <description>Master mode selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>UDE</name>
              <description>Update DMA request enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Low counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Low Auto-reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="TIM6">
      <name>TIM7</name>
      <baseAddress>0x40000C00</baseAddress>
      <interrupt>
        <name>TIM6_DAC</name>
        <description>TIM6 global interrupt and DAC</description>
        <value>17</value>
      </interrupt>
    </peripheral>
    <peripheral>
      <name>TIM21</name>
      <description>General-purpose-timers</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40010800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM21</name>
        <description>TIMER21 global interrupt</description>
        <value>20</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPM</name>
              <description>One-pulse mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMS</name>
              <description>Center-aligned mode
              selection</description>
              <bitOffset>5</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CKD</name>
              <description>Clock division</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>MMS</name>
              <description>Master mode selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SMCR</name>
          <displayName>SMCR</displayName>
          <description>slave mode control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>SMS</name>
              <description>Slave mode selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TS</name>
              <description>Trigger selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MSM</name>
              <description>Master/Slave mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ETF</name>
              <description>External trigger filter</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ETPS</name>
              <description>External trigger prescaler</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ECE</name>
              <description>External clock enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ETP</name>
              <description>External trigger polarity</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TIE</name>
              <description>Trigger interrupt enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IE</name>
              <description>Capture/Compare 2 interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IE</name>
              <description>Capture/Compare 1 interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC2OF</name>
              <description>Capture/compare 2 overcapture
              flag</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1OF</name>
              <description>Capture/Compare 1 overcapture
              flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIF</name>
              <description>Trigger interrupt flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IF</name>
              <description>Capture/Compare 2 interrupt
              flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IF</name>
              <description>Capture/compare 1 interrupt
              flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TG</name>
              <description>Trigger generation</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2G</name>
              <description>Capture/compare 2
              generation</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1G</name>
              <description>Capture/compare 1
              generation</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Output</name>
          <displayName>CCMR1_Output</displayName>
          <description>capture/compare mode register (output
          mode)</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OC2M</name>
              <description>Output Compare 2 mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC2PE</name>
              <description>Output Compare 2 preload
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC2FE</name>
              <description>Output Compare 2 fast
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OC1M</name>
              <description>Output Compare 1 mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC1PE</name>
              <description>Output Compare 1 preload
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1FE</name>
              <description>Output Compare 1 fast
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Input</name>
          <displayName>CCMR1_Input</displayName>
          <description>capture/compare mode register 1 (input
          mode)</description>
          <alternateRegister>CCMR1_Output</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC2F</name>
              <description>Input capture 2 filter</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC2PSC</name>
              <description>Input capture 2 prescaler</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>IC1F</name>
              <description>Input capture 1 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC1PSC</name>
              <description>Input capture 1 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <displayName>CCER</displayName>
          <description>capture/compare enable
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC2NP</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2P</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2E</name>
              <description>Capture/Compare 2 output
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1NP</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1P</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1E</name>
              <description>Capture/Compare 1 output
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto-reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <displayName>CCR1</displayName>
          <description>capture/compare register 1</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR1</name>
              <description>Capture/Compare 1 value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR2</name>
          <displayName>CCR2</displayName>
          <description>capture/compare register 2</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR2</name>
              <description>Capture/Compare 2 value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OR</name>
          <displayName>OR</displayName>
          <description>TIM21 option register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ETR_RMP</name>
              <description>Timer21 ETR remap</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TI1_RMP</name>
              <description>Timer21 TI1</description>
              <bitOffset>2</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TI2_RMP</name>
              <description>Timer21 TI2</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM22</name>
      <description>General-purpose-timers</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40011400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM22</name>
        <description>TIMER22 global interrupt</description>
        <value>22</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPM</name>
              <description>One-pulse mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMS</name>
              <description>Center-aligned mode
              selection</description>
              <bitOffset>5</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CKD</name>
              <description>Clock division</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>MMS</name>
              <description>Master mode selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SMCR</name>
          <displayName>SMCR</displayName>
          <description>slave mode control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>SMS</name>
              <description>Slave mode selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TS</name>
              <description>Trigger selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MSM</name>
              <description>Master/Slave mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ETF</name>
              <description>External trigger filter</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ETPS</name>
              <description>External trigger prescaler</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ECE</name>
              <description>External clock enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ETP</name>
              <description>External trigger polarity</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TIE</name>
              <description>Trigger interrupt enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IE</name>
              <description>Capture/Compare 2 interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IE</name>
              <description>Capture/Compare 1 interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC2OF</name>
              <description>Capture/compare 2 overcapture
              flag</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1OF</name>
              <description>Capture/Compare 1 overcapture
              flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIF</name>
              <description>Trigger interrupt flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IF</name>
              <description>Capture/Compare 2 interrupt
              flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IF</name>
              <description>Capture/compare 1 interrupt
              flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TG</name>
              <description>Trigger generation</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2G</name>
              <description>Capture/compare 2
              generation</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1G</name>
              <description>Capture/compare 1
              generation</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Output</name>
          <displayName>CCMR1_Output</displayName>
          <description>capture/compare mode register (output
          mode)</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OC2M</name>
              <description>Output Compare 2 mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC2PE</name>
              <description>Output Compare 2 preload
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC2FE</name>
              <description>Output Compare 2 fast
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OC1M</name>
              <description>Output Compare 1 mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC1PE</name>
              <description>Output Compare 1 preload
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1FE</name>
              <description>Output Compare 1 fast
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Input</name>
          <displayName>CCMR1_Input</displayName>
          <description>capture/compare mode register 1 (input
          mode)</description>
          <alternateRegister>CCMR1_Output</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC2F</name>
              <description>Input capture 2 filter</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC2PSC</name>
              <description>Input capture 2 prescaler</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>IC1F</name>
              <description>Input capture 1 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC1PSC</name>
              <description>Input capture 1 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <displayName>CCER</displayName>
          <description>capture/compare enable
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC2NP</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2P</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2E</name>
              <description>Capture/Compare 2 output
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1NP</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1P</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1E</name>
              <description>Capture/Compare 1 output
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto-reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <displayName>CCR1</displayName>
          <description>capture/compare register 1</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR1</name>
              <description>Capture/Compare 1 value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR2</name>
          <displayName>CCR2</displayName>
          <description>capture/compare register 2</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR2</name>
              <description>Capture/Compare 2 value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OR</name>
          <displayName>OR</displayName>
          <description>TIM22 option register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ETR_RMP</name>
              <description>Timer22 ETR remap</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TI1_RMP</name>
              <description>Timer22 TI1</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>LPUSART1</name>
      <description>Universal synchronous asynchronous receiver
      transmitter</description>
      <groupName>USART</groupName>
      <baseAddress>0x40004800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>M1</name>
              <description>Word length</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT4</name>
              <description>Driver Enable assertion
              time</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT3</name>
              <description>DEAT3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT2</name>
              <description>DEAT2</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT1</name>
              <description>DEAT1</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEAT0</name>
              <description>DEAT0</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT4</name>
              <description>Driver Enable de-assertion
              time</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT3</name>
              <description>DEDT3</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT2</name>
              <description>DEDT2</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT1</name>
              <description>DEDT1</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEDT0</name>
              <description>DEDT0</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMIE</name>
              <description>Character match interrupt
              enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MME</name>
              <description>Mute mode enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>M0</name>
              <description>Word length</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WAKE</name>
              <description>Receiver wakeup method</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PCE</name>
              <description>Parity control enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PS</name>
              <description>Parity selection</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PEIE</name>
              <description>PE interrupt enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXEIE</name>
              <description>interrupt enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transmission complete interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXNEIE</name>
              <description>RXNE interrupt enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDLEIE</name>
              <description>IDLE interrupt enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TE</name>
              <description>Transmitter enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RE</name>
              <description>Receiver enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UESM</name>
              <description>USART enable in Stop mode</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UE</name>
              <description>USART enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ADD4_7</name>
              <description>Address of the USART node</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ADD0_3</name>
              <description>Address of the USART node</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSBFIRST</name>
              <description>Most significant bit first</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAINV</name>
              <description>Binary data inversion</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXINV</name>
              <description>TX pin active level
              inversion</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXINV</name>
              <description>RX pin active level
              inversion</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWAP</name>
              <description>Swap TX/RX pins</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOP</name>
              <description>STOP bits</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CLKEN</name>
              <description>Clock enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADDM7</name>
              <description>7-bit Address Detection/4-bit Address
              Detection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR3</name>
          <displayName>CR3</displayName>
          <description>Control register 3</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>WUFIE</name>
              <description>Wakeup from Stop mode interrupt
              enable</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WUS</name>
              <description>Wakeup from Stop mode interrupt flag
              selection</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DEP</name>
              <description>Driver enable polarity
              selection</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DEM</name>
              <description>Driver enable mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DDRE</name>
              <description>DMA Disable on Reception
              Error</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVRDIS</name>
              <description>Overrun Disable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSIE</name>
              <description>CTS interrupt enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSE</name>
              <description>CTS enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RTSE</name>
              <description>RTS enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAT</name>
              <description>DMA enable transmitter</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAR</name>
              <description>DMA enable receiver</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HDSEL</name>
              <description>Half-duplex selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EIE</name>
              <description>Error interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>Baud rate register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>BRR</name>
              <description>BRR</description>
              <bitOffset>0</bitOffset>
              <bitWidth>20</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RQR</name>
          <displayName>RQR</displayName>
          <description>Request register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>RXFRQ</name>
              <description>Receive data flush request</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MMRQ</name>
              <description>Mute mode request</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SBKRQ</name>
              <description>Send break request</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>Interrupt &amp; status
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00C0</resetValue>
          <fields>
            <field>
              <name>REACK</name>
              <description>REACK</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEACK</name>
              <description>TEACK</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WUF</name>
              <description>WUF</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RWU</name>
              <description>RWU</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SBKF</name>
              <description>SBKF</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMF</name>
              <description>CMF</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BUSY</name>
              <description>BUSY</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTS</name>
              <description>CTS</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSIF</name>
              <description>CTSIF</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXE</name>
              <description>TXE</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TC</name>
              <description>TC</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXNE</name>
              <description>RXNE</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDLE</name>
              <description>IDLE</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ORE</name>
              <description>ORE</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NF</name>
              <description>NF</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FE</name>
              <description>FE</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PE</name>
              <description>PE</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>Interrupt flag clear register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>WUCF</name>
              <description>Wakeup from Stop mode clear
              flag</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMCF</name>
              <description>Character match clear flag</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSCF</name>
              <description>CTS clear flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCCF</name>
              <description>Transmission complete clear
              flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDLECF</name>
              <description>Idle line detected clear
              flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ORECF</name>
              <description>Overrun error clear flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NCF</name>
              <description>Noise detected clear flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FECF</name>
              <description>Framing error clear flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PECF</name>
              <description>Parity error clear flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RDR</name>
          <displayName>RDR</displayName>
          <description>Receive data register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>RDR</name>
              <description>Receive data value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>9</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TDR</name>
          <displayName>TDR</displayName>
          <description>Transmit data register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TDR</name>
              <description>Transmit data value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>9</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>NVIC</name>
      <description>Nested Vectored Interrupt
      Controller</description>
      <groupName>NVIC</groupName>
      <baseAddress>0xE000E100</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x33D</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>ISER</name>
          <displayName>ISER</displayName>
          <description>Interrupt Set Enable Register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SETENA</name>
              <description>SETENA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICER</name>
          <displayName>ICER</displayName>
          <description>Interrupt Clear Enable
          Register</description>
          <addressOffset>0x80</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CLRENA</name>
              <description>CLRENA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISPR</name>
          <displayName>ISPR</displayName>
          <description>Interrupt Set-Pending Register</description>
          <addressOffset>0x100</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SETPEND</name>
              <description>SETPEND</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICPR</name>
          <displayName>ICPR</displayName>
          <description>Interrupt Clear-Pending
          Register</description>
          <addressOffset>0x180</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CLRPEND</name>
              <description>CLRPEND</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR0</name>
          <displayName>IPR0</displayName>
          <description>Interrupt Priority Register 0</description>
          <addressOffset>0x300</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRI_0</name>
              <description>priority for interrupt 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_1</name>
              <description>priority for interrupt 1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_2</name>
              <description>priority for interrupt 2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_3</name>
              <description>priority for interrupt 3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR1</name>
          <displayName>IPR1</displayName>
          <description>Interrupt Priority Register 1</description>
          <addressOffset>0x304</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRI_4</name>
              <description>priority for interrupt n</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_5</name>
              <description>priority for interrupt n</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_6</name>
              <description>priority for interrupt n</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_7</name>
              <description>priority for interrupt n</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR2</name>
          <displayName>IPR2</displayName>
          <description>Interrupt Priority Register 2</description>
          <addressOffset>0x308</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRI_8</name>
              <description>priority for interrupt n</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_9</name>
              <description>priority for interrupt n</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_10</name>
              <description>priority for interrupt n</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_11</name>
              <description>priority for interrupt n</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR3</name>
          <displayName>IPR3</displayName>
          <description>Interrupt Priority Register 3</description>
          <addressOffset>0x30C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRI_12</name>
              <description>priority for interrupt n</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_13</name>
              <description>priority for interrupt n</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_14</name>
              <description>priority for interrupt n</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_15</name>
              <description>priority for interrupt n</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR4</name>
          <displayName>IPR4</displayName>
          <description>Interrupt Priority Register 4</description>
          <addressOffset>0x310</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRI_16</name>
              <description>priority for interrupt n</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_17</name>
              <description>priority for interrupt n</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_18</name>
              <description>priority for interrupt n</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_19</name>
              <description>priority for interrupt n</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR5</name>
          <displayName>IPR5</displayName>
          <description>Interrupt Priority Register 5</description>
          <addressOffset>0x314</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRI_20</name>
              <description>priority for interrupt n</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_21</name>
              <description>priority for interrupt n</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_22</name>
              <description>priority for interrupt n</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_23</name>
              <description>priority for interrupt n</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR6</name>
          <displayName>IPR6</displayName>
          <description>Interrupt Priority Register 6</description>
          <addressOffset>0x318</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRI_24</name>
              <description>priority for interrupt n</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_25</name>
              <description>priority for interrupt n</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_26</name>
              <description>priority for interrupt n</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_27</name>
              <description>priority for interrupt n</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR7</name>
          <displayName>IPR7</displayName>
          <description>Interrupt Priority Register 7</description>
          <addressOffset>0x31C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PRI_28</name>
              <description>priority for interrupt n</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_29</name>
              <description>priority for interrupt n</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_30</name>
              <description>priority for interrupt n</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PRI_31</name>
              <description>priority for interrupt n</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
  </peripherals>
</device>
